(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.564)
  )
  (paper "A4")
  (title_block
    (rev "V1.6")
  )
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" power)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "底层丝印层")
    (37 "F.SilkS" user "顶层丝印层")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (44 "Edge.Cuts" user)
    (45 "Margin" user "电气边界")
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 0.48) (material "FR-4") (epsilon_r 4.8) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.017))
      (layer "dielectric 2" (type "prepreg") (thickness 0.48) (material "FR-4") (epsilon_r 4.8) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.017))
      (layer "dielectric 3" (type "core") (thickness 0.48) (material "FR-4") (epsilon_r 4.8) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 46.633799 156.164403)
    (grid_origin 46.633799 156.164403)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "NetR20_1")
  (net 2 "NetC15_2")
  (net 3 "NetP6_2")
  (net 4 "NetP6_1")
  (net 5 "NetP1_2")
  (net 6 "DVP_RST")
  (net 7 "PD22")
  (net 8 "CTP_RST")
  (net 9 "NetR47_1")
  (net 10 "NetC85_1")
  (net 11 "NetC54_2")
  (net 12 "NetDS2_K")
  (net 13 "NetR23_2")
  (net 14 "NetC81_1")
  (net 15 "NetC70_1")
  (net 16 "NetC7_2")
  (net 17 "VCC_RTC")
  (net 18 "TVIN_VRP")
  (net 19 "TVIN_VRN")
  (net 20 "TVIN1")
  (net 21 "TVIN0")
  (net 22 "TV_OUT")
  (net 23 "NetR59_1")
  (net 24 "NetR54_1")
  (net 25 "NetC80_2")
  (net 26 "NetC78_1")
  (net 27 "NetC40_2")
  (net 28 "NetC12_2")
  (net 29 "NetC6_2")
  (net 30 "NetC4_2")
  (net 31 "MICIN3P")
  (net 32 "MICIN3N")
  (net 33 "LINEINR")
  (net 34 "LINEINL")
  (net 35 "AVCC1.8")
  (net 36 "VCC-RMII-CSI")
  (net 37 "NetR50_1")
  (net 38 "NetR35_1")
  (net 39 "DVP_XCLK")
  (net 40 "DVP_VSYNC")
  (net 41 "DVP_SDA")
  (net 42 "DVP_SCL")
  (net 43 "DVP_PCLK")
  (net 44 "DVP_HSYNC")
  (net 45 "DVP_DVDD")
  (net 46 "DVP-Y9")
  (net 47 "DVP-Y8")
  (net 48 "DVP-Y7")
  (net 49 "DVP-Y6")
  (net 50 "DVP-Y5")
  (net 51 "DVP-Y4")
  (net 52 "DVP-Y3")
  (net 53 "DVP-Y2")
  (net 54 "AVDD2V8")
  (net 55 "AAGND")
  (net 56 "PG11")
  (net 57 "CTP_INT")
  (net 58 "WL_REG_ON")
  (net 59 "PB7")
  (net 60 "PB6")
  (net 61 "PB5")
  (net 62 "PB4")
  (net 63 "NetC58_2")
  (net 64 "NetC48_2")
  (net 65 "32I")
  (net 66 "32O")
  (net 67 "XI")
  (net 68 "BT_WAKE_AP")
  (net 69 "BT_EN")
  (net 70 "AP_WAKE_BT")
  (net 71 "D1_P")
  (net 72 "D1_N")
  (net 73 "D0_P")
  (net 74 "D0_N")
  (net 75 "CK_P")
  (net 76 "CK_N")
  (net 77 "NetJ3_B5")
  (net 78 "NetJ3_A5")
  (net 79 "NetJ2_B5")
  (net 80 "NetJ2_A5")
  (net 81 "LCD_PWM")
  (net 82 "LCD_D18")
  (net 83 "NetR39_1")
  (net 84 "WL_WAKE_AP")
  (net 85 "VCC_WIFI")
  (net 86 "UART1_TX")
  (net 87 "UART1_RX")
  (net 88 "UART1_RTS")
  (net 89 "UART1_CTS")
  (net 90 "PG5_SDC1_D3")
  (net 91 "PG4_SDC1_D2")
  (net 92 "PG3_SDC1_D1")
  (net 93 "PG2_SDC1_D0")
  (net 94 "PG1_SDC1_CMD")
  (net 95 "PG0_SDC1_CLK")
  (net 96 "NetR41_2")
  (net 97 "AP-CLK24M-OUT")
  (net 98 "USB1_P")
  (net 99 "USB1_N")
  (net 100 "USB0_P")
  (net 101 "USB0_N")
  (net 102 "TP-Y2")
  (net 103 "TP-Y1")
  (net 104 "TP-X2")
  (net 105 "TP-X1")
  (net 106 "SPI0_WP")
  (net 107 "SPI0_HOLD")
  (net 108 "SDC0_DET")
  (net 109 "RESET")
  (net 110 "NetR49_1")
  (net 111 "NetR43_2")
  (net 112 "HPOUTR")
  (net 113 "HPOUTL")
  (net 114 "HPOUTFB")
  (net 115 "GPADC0")
  (net 116 "VCC-DRAM")
  (net 117 "VCC-CORE")
  (net 118 "XO")
  (net 119 "NetC50_1")
  (net 120 "LDOA-OUT")
  (net 121 "NetR42_2")
  (net 122 "NetR12_2")
  (net 123 "NetR10_2")
  (net 124 "NetR8_2")
  (net 125 "VCCIN")
  (net 126 "VCC3V3")
  (net 127 "NetL3_1")
  (net 128 "NetL2_1")
  (net 129 "NetL1_1")
  (net 130 "NetDS1_K")
  (net 131 "GND")
  (net 132 "AGND")
  (net 133 "LCD_CLK")
  (net 134 "LCD_D10")
  (net 135 "LCD_D11")
  (net 136 "LCD_D12")
  (net 137 "LCD_D13")
  (net 138 "LCD_D14")
  (net 139 "LCD_D15")
  (net 140 "LCD_D19")
  (net 141 "LCD_D20")
  (net 142 "LCD_D21")
  (net 143 "LCD_D22")
  (net 144 "LCD_D23")
  (net 145 "LCD_DE")
  (net 146 "LCD_HSYNC")
  (net 147 "LCD_VSYNC")
  (net 148 "SDC0_CLK")
  (net 149 "SDC0_CMD")
  (net 150 "SDC0_D0")
  (net 151 "SDC0_D1")
  (net 152 "SDC0_D2")
  (net 153 "SDC0_D3")
  (net 154 "SPI0_CLK")
  (net 155 "SPI0_CS")
  (net 156 "SPI0_MISO")
  (net 157 "SPI0_MOSI")
  (net 158 "LEDA")
  (net 159 "LEDK")
  (net 160 "NetD1_A")
  (net 161 "NetC7_1")
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 63.143799 145.928203 90)
    (fp_text reference "C30" (at 1.536702 -0.1143 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at -3.060698 -0.1143 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "VCC-DRAM") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 80.618999 126.141603 90)
    (fp_text reference "C55" (at -1.5367 -3.949705 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at 3.0607 -5.219705 180 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "VCCIN") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 63.778799 126.141603 -90)
    (fp_text reference "C34" (at 1.5367 -0.1143 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -3.0607 -0.1143 180 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:USB-TYPEC-16P" locked (layer "F.Cu")
    (tedit 0)
    (at 54.602599 143.207203 -90)
    (fp_text reference "J2" (at -5.691594 4.952403 unlocked) (layer "F.SilkS") hide)
    (fp_text value "USB-TypeC-16P" (at 6.4897 0.5207 unlocked) (layer "F.SilkS") hide)
    (pad "0" thru_hole oval locked (at 4.319999 -1.632501) (size 2 1) (drill oval 1.5 0.7) (layers *.Cu *.Mask)
      (net 131 "GND"))
    (pad "0" thru_hole oval locked (at -4.319999 2.547501) (size 1.5 1) (drill oval 1.2 0.7) (layers *.Cu *.Mask)
      (net 131 "GND"))
    (pad "0" thru_hole oval locked (at 4.319999 2.547501) (size 1.5 1) (drill oval 1.2 0.7) (layers *.Cu *.Mask)
      (net 131 "GND"))
    (pad "0" thru_hole oval locked (at -4.319999 -1.632501) (size 2 1) (drill oval 1.5 0.7) (layers *.Cu *.Mask)
      (net 131 "GND"))
    (pad "A1" smd rect locked (at -3.400001 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "A4" smd rect locked (at -2.6 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "VCCIN"))
    (pad "A5" smd rect locked (at -1.25 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "NetJ2_A5"))
    (pad "A6" smd rect locked (at -0.25 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "USB1_P"))
    (pad "A7" smd rect locked (at 0.249999 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "USB1_N"))
    (pad "A8" smd rect locked (at 1.25 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "A9" smd rect locked (at 2.6 -2.547501 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "VCCIN"))
    (pad "A12" smd rect locked (at 3.400001 -2.547501 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "B1" smd rect locked (at 3.099999 -2.547501 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "B4" smd rect locked (at 2.3 -2.547501 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "VCCIN"))
    (pad "B5" smd rect locked (at 1.749999 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "NetJ2_B5"))
    (pad "B6" smd rect locked (at 0.750001 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "USB1_P"))
    (pad "B7" smd rect locked (at -0.750001 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "USB1_N"))
    (pad "B8" smd rect locked (at -1.749999 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "B9" smd rect locked (at -2.300001 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "VCCIN"))
    (pad "B12" smd rect locked (at -3.099999 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 66.445799 126.141603 -90)
    (fp_text reference "R66" (at -1.4732 0.0508 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47K" (at 2.9845 0.16506 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "PG5_SDC1_D3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 62.178599 135.768203 90)
    (fp_text reference "C79" (at 1.8855 0.3869 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -2.5595 0.3869 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "LDOA-OUT") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:VLS252010" (layer "F.Cu")
    (tedit 0)
    (at 82.549399 125.684403 180)
    (fp_text reference "L4" (at -1.1811 2.5527 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uH" (at -5.4991 -4.1021 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect (at 0.950001 0 270) (size 2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "VCCIN"))
    (pad "2" smd rect (at -0.95 0 270) (size 2 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "NetD1_A"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 61.746799 142.067403)
    (fp_text reference "R9" (at -0.520698 -1.1303 unlocked) (layer "F.SilkS") hide)
    (fp_text value "150K 1%" (at -0.5207 2.9083 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 124 "NetR8_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 59.359204 138.765403 -90)
    (fp_text reference "C43" (at -4.318002 2.1336 unlocked) (layer "F.SilkS") hide)
    (fp_text value "22pF" (at 0.139698 2.24786 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "32O") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 59.359199 140.594203 -90)
    (fp_text reference "R8" (at -0.520697 -1.1303 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "680K 1%" (at -0.5207 2.9083 -90 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 124 "NetR8_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:XTAL2520" (layer "F.Cu")
    (tedit 0)
    (at 59.714799 136.200003 90)
    (fp_text reference "X1" (at -0.325006 -0.273198 unlocked) (layer "F.SilkS") hide)
    (fp_text value "XTAL2520-24M CL=18PF" (at -8.612899 -2.633698 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at 0.8636 -0.5588 270) (size 0.999998 0.599948) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "XO"))
    (pad "2" smd rect (at -0.8636 -0.5588 270) (size 0.999998 0.599948) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "3" smd rect (at -0.8636 0.5588 270) (size 0.999998 0.599948) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "XI"))
    (pad "4" smd rect (at 0.8636 0.5588 270) (size 0.999998 0.599948) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 78.688599 123.982603 180)
    (fp_text reference "R19" (at 0.0381 1.5367 unlocked) (layer "F.SilkS") hide)
    (fp_text value "2R7" (at 0.0381 -3.0353 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "VCCIN") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "NetC85_1") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 73.633999 126.141603 90)
    (fp_text reference "C70" (at 1.4605 -0.0381 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -2.9845 -0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "NetC70_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 78.726699 126.141603 90)
    (fp_text reference "C15" (at 1.5367 -0.0381 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at -3.0353 -0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "HPOUTR") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "NetC15_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 64.261399 124.490603)
    (fp_text reference "R14" (at 1.282697 0.0127 270 unlocked) (layer "F.SilkS") hide)
    (fp_text value "NC/100K" (at -3.0607 0.0127 270 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "WL_REG_ON") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:TEST-POINT" (layer "F.Cu")
    (tedit 0)
    (at 83.666999 134.422003 -90)
    (fp_text reference "TP5" (at -1.2319 0.2413 unlocked) (layer "F.SilkS") hide)
    (fp_text value "TEST POINT" (at 2.7559 0.2413 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0 270) (size 0.762 0.762) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "LINEINL") (solder_paste_margin -0.4))
  )
  (footprint "LIB_MANGO.IntLib:MIPI_CSI_1.0_30PIN" locked (layer "F.Cu")
    (tedit 0)
    (at 88.002598 135.707203)
    (fp_text reference "P5" (at -0.855388 -11.166046 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Header15-MIPI" (at -1.844832 27.3223 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect locked (at 1.560002 -6.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "1" smd rect locked (at -1.559997 -6.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "2" smd rect locked (at 1.560002 -5.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "D1_N"))
    (pad "2" smd rect locked (at -1.559997 -5.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "D1_N"))
    (pad "3" smd rect locked (at 1.560002 -4.999998) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "D1_P"))
    (pad "3" smd rect locked (at -1.559997 -4.999998) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "D1_P"))
    (pad "4" smd rect locked (at 1.560002 -4) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "4" smd rect locked (at -1.559997 -4) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "5" smd rect locked (at 1.560002 -2.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "CK_N"))
    (pad "5" smd rect locked (at -1.559997 -2.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "CK_N"))
    (pad "6" smd rect locked (at 1.560002 -1.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "CK_P"))
    (pad "6" smd rect locked (at -1.559997 -1.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "CK_P"))
    (pad "7" smd rect locked (at 1.560002 -1.000001) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "7" smd rect locked (at -1.559997 -1.000001) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "8" smd rect locked (at -1.559997 0) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "D0_N"))
    (pad "8" smd rect locked (at 1.560002 0) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "D0_N"))
    (pad "9" smd rect locked (at 1.560002 1) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "D0_P"))
    (pad "9" smd rect locked (at -1.559997 1) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "D0_P"))
    (pad "10" smd rect locked (at -1.559997 1.999998) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "10" smd rect locked (at 1.560002 1.999998) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "11" smd rect locked (at 1.560002 2.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "DVP_SCL"))
    (pad "11" smd rect locked (at -1.559997 2.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "DVP_SCL"))
    (pad "12" smd rect locked (at -1.559997 3.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "DVP_SDA"))
    (pad "12" smd rect locked (at 1.560002 3.999999) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "DVP_SDA"))
    (pad "13" smd rect locked (at -1.559997 4.999997) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "13" smd rect locked (at 1.560002 4.999997) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "14" smd rect locked (at 1.560002 5.999998) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "VCC3V3"))
    (pad "14" smd rect locked (at -1.559997 5.999998) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "VCC3V3"))
    (pad "15" smd rect locked (at 1.560002 6.999998) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "VCC3V3"))
    (pad "15" smd rect locked (at -1.559997 6.999998) (size 1.77 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "VCC3V3"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 83.311399 143.566003 180)
    (fp_text reference "C75" (at 0.072215 1.593662 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1nF" (at 0.072215 -2.851338 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "TP-X1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 63.143799 144.023203 90)
    (fp_text reference "C26" (at 1.5367 -0.1143 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at -3.0607 -0.1143 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "VCCIN") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 64.718599 126.141603 -90)
    (fp_text reference "R5" (at 1.282698 0.0127 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100K" (at -3.0607 0.0127 180 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "WL_REG_ON") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 82.854201 145.902803 90)
    (fp_text reference "R80" (at 1.536705 0.8763 unlocked) (layer "F.SilkS") hide)
    (fp_text value "5.1K" (at -3.035295 0.8763 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.457198 -0.000002 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "NetDS2_K") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "PD22") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:LED0402" (layer "F.Cu")
    (tedit 0)
    (at 52.002599 134.207203 90)
    (fp_text reference "DS1" (at 2.0701 -0.419102 unlocked) (layer "F.SilkS") hide)
    (fp_text value "GREEN" (at -3.5941 -0.419102 unlocked) (layer "F.SilkS") hide)
    (pad "A" smd rect (at -0.507998 0 180) (size 0.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "VCC3V3"))
    (pad "K" smd rect (at 0.507997 0 180) (size 0.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "NetDS1_K"))
  )
  (footprint "D:_ÏîÄ¿_ADLIB_A.Pc_HDR2X11T" locked (layer "F.Cu")
    (tedit 0)
    (at 71.002599 151.707204)
    (fp_text reference "P3" (at -11.0338 -9.990001 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Header 11X2" (at 10.839191 -0.000005 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd oval locked (at -12.7 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "2" smd oval locked (at -12.7 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "VCC3V3"))
    (pad "3" smd oval locked (at -10.16 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "USB1_N"))
    (pad "4" smd oval locked (at -10.16 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "USB1_P"))
    (pad "5" smd oval locked (at -7.62 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "DVP_HSYNC"))
    (pad "6" smd oval locked (at -7.62 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "DVP_VSYNC"))
    (pad "7" smd oval locked (at -5.08 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "DVP_PCLK"))
    (pad "8" smd oval locked (at -5.08 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "DVP_XCLK"))
    (pad "9" smd oval locked (at -2.54 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "DVP-Y2"))
    (pad "10" smd oval locked (at -2.54 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "DVP-Y3"))
    (pad "11" smd oval locked (at 0 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "DVP-Y4"))
    (pad "12" smd oval locked (at 0 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "DVP-Y5"))
    (pad "13" smd oval locked (at 2.54 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "DVP-Y6"))
    (pad "14" smd oval locked (at 2.54 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "DVP-Y7"))
    (pad "15" smd oval locked (at 5.08 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "DVP-Y8"))
    (pad "16" smd oval locked (at 5.08 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "DVP-Y9"))
    (pad "17" smd oval locked (at 7.62 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "DVP_SCL"))
    (pad "18" smd oval locked (at 7.62 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "DVP_SDA"))
    (pad "19" smd oval locked (at 10.16 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "CTP_RST"))
    (pad "20" smd oval locked (at 10.16 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "CTP_INT"))
    (pad "21" smd oval locked (at 12.7 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "PB4"))
    (pad "22" smd oval locked (at 12.7 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "PB5"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 75.030999 126.141603 -90)
    (fp_text reference "R29" (at 1.5367 -0.1143 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100K" (at -3.0607 -0.1143 180 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "GPADC0") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "AVCC1.8") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:I-PEX SOCKET" locked (layer "F.Cu")
    (tedit 0)
    (at 60.425999 127.310003 180)
    (fp_text reference "J4" (at 1.301603 2.773794 unlocked) (layer "F.SilkS") hide)
    (fp_text value "ipex" (at 1.7653 -3.8481 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect locked (at 0 1.549999 270) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "NetC48_2"))
    (pad "2" smd rect locked (at 1.4 0 270) (size 2.2 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "3" smd rect locked (at -1.399999 0 270) (size 2.2 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 61.746799 141.051403 180)
    (fp_text reference "C68" (at -1.625846 0.456542 270 unlocked) (layer "F.SilkS") hide)
    (fp_text value "2.2uF" (at 0.0381 -2.9845 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 78.688599 124.846203)
    (fp_text reference "R21" (at -0.0381 -1.5367 unlocked) (layer "F.SilkS") hide)
    (fp_text value "150K 1%" (at -0.0381 3.2893 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "NetR20_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "NetC15_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 69.036599 126.141603 -90)
    (fp_text reference "R68" (at -1.4732 0.0508 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47K" (at 2.9845 0.16506 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "PG2_SDC1_D0") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 67.283999 126.141603 -90)
    (fp_text reference "R69" (at -1.4732 0.0508 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47K" (at 2.9845 0.16506 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "PG3_SDC1_D1") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 75.919999 126.141603 90)
    (fp_text reference "C49" (at 1.5367 -0.1143 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1nF" (at -3.0607 -0.1143 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 132 "AGND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "GPADC0") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 82.854199 142.169003 90)
    (fp_text reference "C35" (at 1.282697 0.0127 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -2.8067 0.012702 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 61.264199 137.419203 90)
    (fp_text reference "C9" (at 1.282697 0.012702 unlocked) (layer "F.SilkS") hide)
    (fp_text value "22pF" (at -2.8067 0.012702 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "XI") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "D:_×ÊÁÏ¿â_ADLIB_A.PcbLib_HDR2X11T" locked (layer "F.Cu")
    (tedit 0)
    (at 71.002599 119.707204)
    (fp_text reference "P2" (at -0.990188 -4.310047 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Header 11X2" (at -3.047014 0 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval locked (at -12.7 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "2" smd oval locked (at -12.7 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "VCC3V3"))
    (pad "3" smd oval locked (at -10.16 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "PG0_SDC1_CLK"))
    (pad "4" smd oval locked (at -10.16 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "PG1_SDC1_CMD"))
    (pad "5" smd oval locked (at -7.62 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "PG2_SDC1_D0"))
    (pad "6" smd oval locked (at -7.62 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "PG3_SDC1_D1"))
    (pad "7" smd oval locked (at -5.08 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "PG4_SDC1_D2"))
    (pad "8" smd oval locked (at -5.08 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "PG5_SDC1_D3"))
    (pad "9" smd oval locked (at -2.54 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "UART1_TX"))
    (pad "10" smd oval locked (at -2.54 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "UART1_RX"))
    (pad "11" smd oval locked (at 0 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "UART1_RTS"))
    (pad "12" smd oval locked (at 0 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "UART1_CTS"))
    (pad "13" smd oval locked (at 2.54 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "WL_WAKE_AP"))
    (pad "14" smd oval locked (at 2.54 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "PG11"))
    (pad "15" smd oval locked (at 5.08 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "WL_REG_ON"))
    (pad "16" smd oval locked (at 5.08 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "AP_WAKE_BT"))
    (pad "17" smd oval locked (at 7.62 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "BT_WAKE_AP"))
    (pad "18" smd oval locked (at 7.62 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "BT_EN"))
    (pad "19" smd oval locked (at 10.16 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "PD22"))
    (pad "20" smd oval locked (at 10.16 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "GPADC0"))
    (pad "21" smd oval locked (at 12.7 2.749997) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "VCCIN"))
    (pad "22" smd oval locked (at 12.7 -2.750002) (size 0.8 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 60.273599 138.765403 -90)
    (fp_text reference "R40" (at -1.071994 0.438003 unlocked) (layer "F.SilkS") hide)
    (fp_text value "680K 1%" (at 2.9845 0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "32O") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "32I") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 88.002598 119.707204)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "2" thru_hole circle (at 0 0) (size 5.334 5.334) (drill 2.7) (layers *.Cu *.Mask)
      (net 131 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 80.263399 142.169003 90)
    (fp_text reference "C20" (at -1.7907 -3.8227 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at 3.3147 -6.6167 180 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 76.859799 126.141603 90)
    (fp_text reference "C6" (at -0.248806 -0.400198 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 4.172498 12.496299 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "HPOUTR") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "NetC6_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:SOD523" (layer "F.Cu")
    (tedit 0)
    (at 82.498599 127.741803)
    (fp_text reference "D1" (at -1.079498 1.3081 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "MSK4010" (at -8.953498 -2.8321 180 unlocked) (layer "B.SilkS") hide)
    (pad "A" smd rect (at -0.749999 -0.000002 90) (size 0.9 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "NetD1_A"))
    (pad "K" smd rect (at 0.750001 -0.000002 90) (size 0.9 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "LEDA"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 66.902999 124.516003)
    (fp_text reference "C18" (at 1.161003 2.103006 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "NC" (at -0.856973 0.713499 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "PG0_SDC1_CLK") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 64.083599 145.928203 -90)
    (fp_text reference "C31" (at 1.5367 -0.1143 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -3.0607 -0.1143 180 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "VCC-DRAM") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 58.343199 132.618603 180)
    (fp_text reference "R48" (at -1.321458 -0.787154 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10K" (at 0.672895 -2.9845 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "SDC0_DET") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 62.178599 137.419203 90)
    (fp_text reference "C8" (at 1.282697 0.0127 unlocked) (layer "F.SilkS") hide)
    (fp_text value "22pF" (at -2.8067 0.012702 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "XO") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 70.763799 126.141603 -90)
    (fp_text reference "C10" (at -1.7907 -3.8227 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at 3.3147 -6.6167 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "VCC-CORE") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 85.749799 125.684403 -90)
    (fp_text reference "R16" (at -1.5367 0.0381 unlocked) (layer "F.SilkS") hide)
    (fp_text value "75R" (at 3.0353 0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "NetP1_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 158 "LEDA") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 78.967999 143.388203 180)
    (fp_text reference "C13" (at -1.7907 -3.5687 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at 3.3147 -6.3627 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "LDOA-OUT") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 62.457999 124.516003)
    (fp_text reference "R70" (at 1.193802 -0.279402 unlocked) (layer "F.SilkS") hide)
    (fp_text value "NC/100K" (at -1.840512 4.178298 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "UART1_CTS") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 62.178599 139.679803 -90)
    (fp_text reference "R61" (at -1.73513 0.768988 45 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0R" (at 2.9845 0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "VCC_RTC") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "LDOA-OUT") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 85.425423 144.957179)
    (fp_text reference "C73" (at -0.0381 -1.4605 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1nF" (at -0.0381 2.9845 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "TP-Y1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:TEST-POINT" (layer "F.Cu")
    (tedit 0)
    (at 80.898399 135.806303 90)
    (fp_text reference "TP1" (at 1.2319 -0.2413 unlocked) (layer "F.SilkS") hide)
    (fp_text value "TEST POINT" (at -2.7559 -0.2413 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0 90) (size 0.762 0.762) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "TV_OUT") (solder_paste_margin -0.4))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 54.533199 134.879203 180)
    (fp_text reference "R18" (at 1.282698 0.0127 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10K" (at -2.8067 0.012702 90 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 149 "SDC0_CMD") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 84.809999 141.280003 90)
    (fp_text reference "C3" (at -1.7653 1.2573 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -5.829295 -2.7813 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 80.415799 137.901803)
    (fp_text reference "R59" (at -0.0381 -1.4605 unlocked) (layer "F.SilkS") hide)
    (fp_text value "33R" (at -0.0381 2.9845 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "NetR59_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 133 "LCD_CLK") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:TEST-POINT" (layer "F.Cu")
    (tedit 0)
    (at 82.244599 135.806303 90)
    (fp_text reference "TP2" (at 1.2319 -0.2413 unlocked) (layer "F.SilkS") hide)
    (fp_text value "TEST POINT" (at -2.7559 -0.2413 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0 90) (size 0.762 0.762) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND") (solder_paste_margin -0.4))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 83.311399 144.480403 180)
    (fp_text reference "C74" (at 0.28796 2.114517 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1nF" (at 0.28796 -2.330483 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "TP-X2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 58.470199 140.594203 90)
    (fp_text reference "C27" (at 1.5367 -0.1143 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at -3.0607 -0.1143 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "VCCIN") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0603" (layer "F.Cu")
    (tedit 0)
    (at 84.708399 125.684403 90)
    (fp_text reference "C1" (at 0.6223 -0.9525 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1uF 50V" (at -3.0353 -0.9525 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.635 0 270) (size 0.8001 0.849884) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "LEDA"))
    (pad "2" smd rect (at 0.635 0 270) (size 0.8001 0.849884) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/User Library-0603 SMD Capacitor.STEP"
      (offset (xyz -0.000041 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:Y3215" (layer "F.Cu")
    (tedit 0)
    (at 57.250999 136.200003 90)
    (fp_text reference "XT1" (at 2.0828 -1.8288 unlocked) (layer "F.SilkS") hide)
    (fp_text value "32.768K CL=12.5pF" (at -2.705182 -12.861527 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -1.25 0 270) (size 1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "32I"))
    (pad "2" smd rect (at 1.25 0 90) (size 1 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "32O"))
  )
  (footprint "LIB_MANGO.IntLib:USB-TYPEC-16P" locked (layer "F.Cu")
    (tedit 0)
    (at 54.602599 128.207202 -90)
    (fp_text reference "J3" (at -0.170401 7.5184 unlocked) (layer "F.SilkS") hide)
    (fp_text value "USB-TypeC-16P" (at 6.4897 0.5207 unlocked) (layer "F.SilkS") hide)
    (pad "0" thru_hole oval locked (at -4.319999 2.547501) (size 1.5 1) (drill oval 1.2 0.7) (layers *.Cu *.Mask)
      (net 131 "GND"))
    (pad "0" thru_hole oval locked (at 4.319999 2.547501) (size 1.5 1) (drill oval 1.2 0.7) (layers *.Cu *.Mask)
      (net 131 "GND"))
    (pad "0" thru_hole oval locked (at 4.319999 -1.632501) (size 2 1) (drill oval 1.5 0.7) (layers *.Cu *.Mask)
      (net 131 "GND"))
    (pad "0" thru_hole oval locked (at -4.319999 -1.632501) (size 2 1) (drill oval 1.5 0.7) (layers *.Cu *.Mask)
      (net 131 "GND"))
    (pad "A1" smd rect locked (at -3.4 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "A4" smd rect locked (at -2.599999 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "VCCIN"))
    (pad "A5" smd rect locked (at -1.25 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "NetJ3_A5"))
    (pad "A6" smd rect locked (at -0.249999 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "USB0_P"))
    (pad "A7" smd rect locked (at 0.25 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "USB0_N"))
    (pad "A8" smd rect locked (at 1.25 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "A9" smd rect locked (at 2.6 -2.547501 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "VCCIN"))
    (pad "A12" smd rect locked (at 3.400001 -2.547501 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "B1" smd rect locked (at 3.099999 -2.547501 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "B4" smd rect locked (at 2.300001 -2.547501 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "VCCIN"))
    (pad "B5" smd rect locked (at 1.749999 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "NetJ3_B5"))
    (pad "B6" smd rect locked (at 0.750001 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "USB0_P"))
    (pad "B7" smd rect locked (at -0.750001 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "USB0_N"))
    (pad "B8" smd rect locked (at -1.749999 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "B9" smd rect locked (at -2.3 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "VCCIN"))
    (pad "B12" smd rect locked (at -3.099998 -2.547501 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:HDR1X2-XIAO" locked (layer "F.Cu")
    (tedit 0)
    (at 86.791199 147.707204)
    (fp_text reference "P8" (at -2.241403 -1.351395 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Header 2" (at 0.2921 5.4229 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 60 "PB6"))
    (pad "2" thru_hole circle locked (at 2.54 0) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 59 "PB7"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 71.043199 124.516003)
    (fp_text reference "R41" (at -0.438003 -1.071994 unlocked) (layer "F.SilkS") hide)
    (fp_text value "NC/0R" (at -1.3843 2.4003 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "AP-CLK24M-OUT") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "NetR41_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 79.679199 126.141603 -90)
    (fp_text reference "C86" (at -1.5367 0.0381 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 3.0353 0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 132 "AGND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "HPOUTFB") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:QFN40P300X300X80_HS-21N" locked (layer "F.Cu")
    (tedit 0)
    (at 60.6282 144.924799 90)
    (fp_text reference "U4" (at -0.749298 2.8067 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "RY1303" (at -6.8453 -4.3307 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd oval locked (at -1.525001 -0.8 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "2" smd oval locked (at -1.525001 -0.400001 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "NetR12_2"))
    (pad "3" smd oval locked (at -1.525001 0 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "NetR10_2"))
    (pad "4" smd oval locked (at -1.525001 0.4 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "5" smd oval locked (at -1.525001 0.799999 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "6" smd oval locked (at -0.800001 1.524999 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "NetL3_1"))
    (pad "7" smd oval locked (at -0.400002 1.524999 90) (size 0.2 0.762) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "VCCIN"))
    (pad "8" smd oval locked (at 0 1.524999 90) (size 0.2 0.635) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "NetR23_2"))
    (pad "9" smd oval locked (at 0.399999 1.524999 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "VCCIN"))
    (pad "10" smd oval locked (at 0.799998 1.524999 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "VCCIN"))
    (pad "11" smd oval locked (at 1.524998 0.799999 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "NetL1_1"))
    (pad "12" smd oval locked (at 1.524998 0.4 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "13" smd oval locked (at 1.524998 0 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "14" smd oval locked (at 1.524998 -0.400001 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "NetR8_2"))
    (pad "15" smd oval locked (at 1.524998 -0.8 180) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "16" smd oval locked (at 0.799998 -1.525 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "VCCIN"))
    (pad "17" smd oval locked (at 0.399999 -1.525 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
    (pad "18" smd oval locked (at 0 -1.525 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "NetC4_2"))
    (pad "19" smd oval locked (at -0.400002 -1.525 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "VCCIN"))
    (pad "20" smd oval locked (at -0.800001 -1.525 90) (size 0.2 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "NetL2_1"))
    (pad "21" smd rect locked (at 0 0 90) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 88.002598 151.707204)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "2" thru_hole circle (at 0 0) (size 5.334 5.334) (drill 2.7) (layers *.Cu *.Mask)
      (net 131 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:TEST-POINT" (layer "F.Cu")
    (tedit 0)
    (at 82.244599 134.422003 -90)
    (fp_text reference "TP6" (at -1.2319 0.2413 unlocked) (layer "F.SilkS") hide)
    (fp_text value "TEST POINT" (at 2.7559 0.2413 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0 270) (size 0.762 0.762) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "LINEINR") (solder_paste_margin -0.4))
  )
  (footprint "LIB_MANGO.IntLib:TEST-POINT" (layer "F.Cu")
    (tedit 0)
    (at 80.898399 134.422003 -90)
    (fp_text reference "TP7" (at -1.2319 0.2413 unlocked) (layer "F.SilkS") hide)
    (fp_text value "TEST POINT" (at 2.7559 0.2413 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle (at 0 0 270) (size 0.762 0.762) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "AGND") (solder_paste_margin -0.4))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 85.425423 145.902803)
    (fp_text reference "C72" (at -0.0381 -1.4605 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1nF" (at -0.0381 2.9845 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "TP-Y2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 65.582199 126.141603 -90)
    (fp_text reference "R65" (at -1.4732 0.0508 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47K" (at 2.9845 0.16506 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "PG4_SDC1_D2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 69.950999 126.141603 -90)
    (fp_text reference "R67" (at -1.4732 0.0508 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47K" (at 2.9845 0.16506 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "PG1_SDC1_CMD") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 61.772199 132.618603)
    (fp_text reference "R43" (at -0.438003 -1.071994 unlocked) (layer "F.SilkS") hide)
    (fp_text value "33R" (at -0.0381 2.9845 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 148 "SDC0_CLK") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000002) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "NetR43_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:HDR1X2-XIAO" locked (layer "F.Cu")
    (tedit 0)
    (at 86.791199 123.707204)
    (fp_text reference "P6" (at -1.733403 -1.478395 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Header 2" (at -1.7145 2.9845 unlocked) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 4 "NetP6_1"))
    (pad "2" thru_hole circle locked (at 2.54 0) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 3 "NetP6_2"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 54.002598 119.707204)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "2" thru_hole circle (at 0 0) (size 5.334 5.334) (drill 2.7) (layers *.Cu *.Mask)
      (net 131 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 63.626399 147.249003 180)
    (fp_text reference "R10" (at 1.536703 -0.114298 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "300K 1%" (at -3.3147 -0.114298 90 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "VCC-DRAM") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "NetR10_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 54.533199 136.530203)
    (fp_text reference "C41" (at 1.5367 -0.1143 270 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -3.0607 -0.1143 270 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:QFP129P40B1600_1600H160" locked (layer "F.Cu")
    (tedit 0)
    (at 71.002599 135.707203 -90)
    (fp_text reference "U1" (at 0.723897 5.0419 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "D1s-eLQFP128" (at -1.3081 -6.769103 90 unlocked) (layer "B.SilkS") hide)
    (fp_text user "94" (at -5.439989 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "42" (at 7.409998 2.399995 90 unlocked) (layer "Eco1.User"))
    (fp_text user "20" (at 1.359997 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "53" (at 7.409998 -1.999996 90 unlocked) (layer "Eco1.User"))
    (fp_text user "64" (at 7.409998 -6.400013 90 unlocked) (layer "Eco1.User"))
    (fp_text user "73" (at 2.959994 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "115" (at -8.009997 0.799998 90 unlocked) (layer "Eco1.User"))
    (fp_text user "12" (at -1.839997 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "62" (at 7.409998 -5.599989 90 unlocked) (layer "Eco1.User"))
    (fp_text user "114" (at -8.009997 0.399999 90 unlocked) (layer "Eco1.User"))
    (fp_text user "128" (at -8.009997 5.999988 90 unlocked) (layer "Eco1.User"))
    (fp_text user "86" (at -2.239996 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "120" (at -8.009997 2.799994 90 unlocked) (layer "Eco1.User"))
    (fp_text user "52" (at 7.409998 -1.599997 90 unlocked) (layer "Eco1.User"))
    (fp_text user "33" (at 7.409998 5.999988 90 unlocked) (layer "Eco1.User"))
    (fp_text user "100" (at -8.009997 -5.19999 90 unlocked) (layer "Eco1.User"))
    (fp_text user "121" (at -8.009997 3.199993 90 unlocked) (layer "Eco1.User"))
    (fp_text user "66" (at 5.759988 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "118" (at -8.009997 1.999996 90 unlocked) (layer "Eco1.User"))
    (fp_text user "9" (at -2.919995 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "109" (at -8.009997 -1.599997 90 unlocked) (layer "Eco1.User"))
    (fp_text user "83" (at -1.039998 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "71" (at 3.759992 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "57" (at 7.409998 -3.599993 90 unlocked) (layer "Eco1.User"))
    (fp_text user "98" (at -7.889997 -5.999988 90 unlocked) (layer "Eco1.User"))
    (fp_text user "46" (at 7.409998 0.799998 90 unlocked) (layer "Eco1.User"))
    (fp_text user "104" (at -8.009997 -3.599993 90 unlocked) (layer "Eco1.User"))
    (fp_text user "87" (at -2.639995 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "F133-eLQFP128" (at -1.070001 0.259994 -90 unlocked) (layer "Eco1.User"))
    (fp_text user "129" (at -0.344993 0.083007 -90 unlocked) (layer "Eco1.User"))
    (fp_text user "74" (at 2.559995 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "2" (at -5.719989 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "29" (at 4.95999 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "101" (at -8.009997 -4.799991 90 unlocked) (layer "Eco1.User"))
    (fp_text user "36" (at 7.409998 4.79999 90 unlocked) (layer "Eco1.User"))
    (fp_text user "40" (at 7.409998 3.199993 90 unlocked) (layer "Eco1.User"))
    (fp_text user "81" (at -0.24 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "44" (at 7.409998 1.599996 90 unlocked) (layer "Eco1.User"))
    (fp_text user "84" (at -1.439997 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "30" (at 5.359989 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "24" (at 2.959994 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "76" (at 1.759996 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "123" (at -8.009997 3.999992 90 unlocked) (layer "Eco1.User"))
    (fp_text user "4" (at -4.919991 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "56" (at 7.409998 -3.199994 90 unlocked) (layer "Eco1.User"))
    (fp_text user "99" (at -7.889997 -5.599989 90 unlocked) (layer "Eco1.User"))
    (fp_text user "111" (at -8.009997 -0.799999 90 unlocked) (layer "Eco1.User"))
    (fp_text user "28" (at 4.559991 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "70" (at 4.159991 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "14" (at -1.039998 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "32" (at 6.160013 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "85" (at -1.839997 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "96" (at -6.239988 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "106" (at -8.009997 -2.799995 90 unlocked) (layer "Eco1.User"))
    (fp_text user "5" (at -4.519991 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "21" (at 1.759996 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "124" (at -8.009997 4.399991 90 unlocked) (layer "Eco1.User"))
    (fp_text user "17" (at 0.159999 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "91" (at -4.239992 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "10" (at -2.639995 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "50" (at 7.409998 -0.799999 90 unlocked) (layer "Eco1.User"))
    (fp_text user "77" (at 1.359997 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "3" (at -5.31999 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "90" (at -3.839993 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "13" (at -1.439997 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "89" (at -3.439993 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "113" (at -8.009997 0 90 unlocked) (layer "Eco1.User"))
    (fp_text user "107" (at -8.009997 -2.399996 90 unlocked) (layer "Eco1.User"))
    (fp_text user "48" (at 7.409998 0 90 unlocked) (layer "Eco1.User"))
    (fp_text user "79" (at 0.559999 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "127" (at -8.009997 5.599988 90 unlocked) (layer "Eco1.User"))
    (fp_text user "59" (at 7.409998 -4.399992 90 unlocked) (layer "Eco1.User"))
    (fp_text user "49" (at 7.409998 -0.4 90 unlocked) (layer "Eco1.User"))
    (fp_text user "78" (at 0.959998 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "22" (at 2.159995 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "1" (at -6.119988 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "61" (at 7.409998 -5.19999 90 unlocked) (layer "Eco1.User"))
    (fp_text user "67" (at 5.359989 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "16" (at -0.24 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "23" (at 2.559995 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "37" (at 7.409998 4.399991 90 unlocked) (layer "Eco1.User"))
    (fp_text user "54" (at 7.409998 -2.399996 90 unlocked) (layer "Eco1.User"))
    (fp_text user "122" (at -8.009997 3.599992 90 unlocked) (layer "Eco1.User"))
    (fp_text user "103" (at -8.009997 -3.999992 90 unlocked) (layer "Eco1.User"))
    (fp_text user "18" (at 0.559999 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "112" (at -8.009997 -0.4 90 unlocked) (layer "Eco1.User"))
    (fp_text user "51" (at 7.409998 -1.199998 90 unlocked) (layer "Eco1.User"))
    (fp_text user "75" (at 2.159995 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "110" (at -8.009997 -1.199998 90 unlocked) (layer "Eco1.User"))
    (fp_text user "116" (at -8.009997 1.199997 90 unlocked) (layer "Eco1.User"))
    (fp_text user "69" (at 4.559991 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "11" (at -2.239996 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "119" (at -8.009997 2.399995 90 unlocked) (layer "Eco1.User"))
    (fp_text user "31" (at 5.759988 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "8" (at -3.319994 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "60" (at 7.409998 -4.799991 90 unlocked) (layer "Eco1.User"))
    (fp_text user "88" (at -3.039994 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "43" (at 7.409998 1.999996 90 unlocked) (layer "Eco1.User"))
    (fp_text user "117" (at -8.009997 1.599996 90 unlocked) (layer "Eco1.User"))
    (fp_text user "95" (at -5.839989 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "108" (at -8.009997 -1.999996 90 unlocked) (layer "Eco1.User"))
    (fp_text user "38" (at 7.409998 3.999992 90 unlocked) (layer "Eco1.User"))
    (fp_text user "80" (at 0.159999 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "125" (at -8.009997 4.79999 90 unlocked) (layer "Eco1.User"))
    (fp_text user "93" (at -5.03999 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "34" (at 7.409998 5.599988 90 unlocked) (layer "Eco1.User"))
    (fp_text user "45" (at 7.409998 1.199997 90 unlocked) (layer "Eco1.User"))
    (fp_text user "68" (at 4.95999 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "126" (at -8.009997 5.199989 90 unlocked) (layer "Eco1.User"))
    (fp_text user "65" (at 6.160013 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "63" (at 7.409998 -5.999988 90 unlocked) (layer "Eco1.User"))
    (fp_text user "82" (at -0.639999 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "25" (at 3.359993 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "47" (at 7.409998 0.399999 90 unlocked) (layer "Eco1.User"))
    (fp_text user "35" (at 7.409998 5.199989 90 unlocked) (layer "Eco1.User"))
    (fp_text user "92" (at -4.639991 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "102" (at -8.009997 -4.399992 90 unlocked) (layer "Eco1.User"))
    (fp_text user "19" (at 0.959998 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "26" (at 3.759992 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "15" (at -0.639999 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "105" (at -8.009997 -3.199994 90 unlocked) (layer "Eco1.User"))
    (fp_text user "27" (at 4.159991 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "6" (at -4.119992 7.649997 unlocked) (layer "Eco1.User"))
    (fp_text user "72" (at 3.359993 -7.649998 unlocked) (layer "Eco1.User"))
    (fp_text user "41" (at 7.409998 2.799994 90 unlocked) (layer "Eco1.User"))
    (fp_text user "97" (at -7.889997 -6.400013 90 unlocked) (layer "Eco1.User"))
    (fp_text user "39" (at 7.409998 3.599992 90 unlocked) (layer "Eco1.User"))
    (fp_text user "58" (at 7.409998 -3.999992 90 unlocked) (layer "Eco1.User"))
    (fp_text user "55" (at 7.409998 -2.799995 90 unlocked) (layer "Eco1.User"))
    (fp_text user "7" (at -3.719993 7.649997 unlocked) (layer "Eco1.User"))
    (pad "1" smd oval locked (at -6.199988 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "UART1_TX"))
    (pad "2" smd oval locked (at -5.799989 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "UART1_RX"))
    (pad "3" smd oval locked (at -5.39999 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "UART1_RTS"))
    (pad "4" smd oval locked (at -4.99999 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "UART1_CTS"))
    (pad "5" smd oval locked (at -4.599991 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "WL_WAKE_AP"))
    (pad "6" smd oval locked (at -4.199992 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "PG11"))
    (pad "7" smd oval locked (at -3.799993 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "SDC0_D1"))
    (pad "8" smd oval locked (at -3.399994 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "SDC0_D0"))
    (pad "9" smd oval locked (at -2.999994 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "NetR43_2"))
    (pad "10" smd oval locked (at -2.599995 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "SDC0_CMD"))
    (pad "11" smd oval locked (at -2.199996 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "SDC0_D3"))
    (pad "12" smd oval locked (at -1.799997 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "SDC0_D2"))
    (pad "13" smd oval locked (at -1.399998 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "SDC0_DET"))
    (pad "14" smd oval locked (at -0.999998 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "SPI0_HOLD"))
    (pad "15" smd oval locked (at -0.599999 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "SPI0_WP"))
    (pad "16" smd oval locked (at -0.2 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "SPI0_MISO"))
    (pad "17" smd oval locked (at 0.199999 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "SPI0_MOSI"))
    (pad "18" smd oval locked (at 0.599998 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "SPI0_CS"))
    (pad "19" smd oval locked (at 0.999998 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "NetR49_1"))
    (pad "20" smd oval locked (at 1.399997 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "LDOA-OUT"))
    (pad "21" smd oval locked (at 1.799996 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "AP-CLK24M-OUT"))
    (pad "22" smd oval locked (at 2.199995 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "XO"))
    (pad "23" smd oval locked (at 2.599994 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "XI"))
    (pad "24" smd oval locked (at 2.999994 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "32O"))
    (pad "25" smd oval locked (at 3.399993 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "32I"))
    (pad "26" smd oval locked (at 3.799992 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "VCC_RTC"))
    (pad "27" smd oval locked (at 4.199991 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "RESET"))
    (pad "28" smd oval locked (at 4.59999 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "LDOA-OUT"))
    (pad "29" smd oval locked (at 4.99999 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "VCC3V3"))
    (pad "30" smd oval locked (at 5.399989 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "NetC50_1"))
    (pad "31" smd oval locked (at 5.799988 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "DVP_SDA"))
    (pad "32" smd oval locked (at 6.199987 7.649997 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "DVP_SCL"))
    (pad "33" smd oval locked (at 7.649997 6.199987 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "DVP_XCLK"))
    (pad "34" smd oval locked (at 7.649997 5.799988 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "VCC-RMII-CSI"))
    (pad "35" smd oval locked (at 7.649997 5.399989 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "DVP_PCLK"))
    (pad "36" smd oval locked (at 7.649997 4.99999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "DVP-Y9"))
    (pad "37" smd oval locked (at 7.649997 4.59999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "DVP-Y8"))
    (pad "38" smd oval locked (at 7.649997 4.199991 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "DVP-Y7"))
    (pad "39" smd oval locked (at 7.649997 3.799992 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "DVP-Y6"))
    (pad "40" smd oval locked (at 7.649997 3.399993 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "DVP-Y5"))
    (pad "41" smd oval locked (at 7.649997 2.999994 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "DVP-Y4"))
    (pad "42" smd oval locked (at 7.649997 2.599994 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "DVP-Y3"))
    (pad "43" smd oval locked (at 7.649997 2.199995 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "DVP-Y2"))
    (pad "44" smd oval locked (at 7.649997 1.799996 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "DVP_HSYNC"))
    (pad "45" smd oval locked (at 7.649997 1.399997 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "DVP_VSYNC"))
    (pad "46" smd oval locked (at 7.649997 0.999998 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "VCC-CORE"))
    (pad "47" smd oval locked (at 7.649997 0.599998 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "NetR42_2"))
    (pad "48" smd oval locked (at 7.649997 0.199999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "VCC-DRAM"))
    (pad "49" smd oval locked (at 7.649997 -0.2 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "VCC-DRAM"))
    (pad "50" smd oval locked (at 7.649997 -0.599999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "LDOA-OUT"))
    (pad "51" smd oval locked (at 7.649997 -0.999998 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "VCC-CORE"))
    (pad "52" smd oval locked (at 7.649997 -1.399998 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "PD22"))
    (pad "53" smd oval locked (at 7.649997 -1.799997 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "LCD_VSYNC"))
    (pad "54" smd oval locked (at 7.649997 -2.199996 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "LCD_HSYNC"))
    (pad "55" smd oval locked (at 7.649997 -2.599995 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "D0_P"))
    (pad "56" smd oval locked (at 7.649997 -2.999994 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "D0_N"))
    (pad "57" smd oval locked (at 7.649997 -3.399994 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "D1_P"))
    (pad "58" smd oval locked (at 7.649997 -3.799993 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "D1_N"))
    (pad "59" smd oval locked (at 7.649997 -4.199992 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "CK_P"))
    (pad "60" smd oval locked (at 7.649997 -4.599991 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "CK_N"))
    (pad "61" smd oval locked (at 7.649997 -4.99999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "LCD_D10"))
    (pad "62" smd oval locked (at 7.649997 -5.39999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "LCD_D11"))
    (pad "63" smd oval locked (at 7.649997 -5.799989 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "LCD_D12"))
    (pad "64" smd oval locked (at 7.649997 -6.199988 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "LCD_D13"))
    (pad "65" smd oval locked (at 6.199987 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "LDOA-OUT"))
    (pad "66" smd oval locked (at 5.799988 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "VCC3V3"))
    (pad "67" smd oval locked (at 5.399989 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "LCD_D14"))
    (pad "68" smd oval locked (at 4.99999 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "LCD_D15"))
    (pad "69" smd oval locked (at 4.59999 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "LCD_D19"))
    (pad "70" smd oval locked (at 4.199991 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "LCD_D18"))
    (pad "71" smd oval locked (at 3.799992 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "LCD_D20"))
    (pad "72" smd oval locked (at 3.399993 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "LCD_D21"))
    (pad "73" smd oval locked (at 2.999994 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 143 "LCD_D22"))
    (pad "74" smd oval locked (at 2.599994 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "LCD_D23"))
    (pad "75" smd oval locked (at 2.199995 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "NetR59_1"))
    (pad "76" smd oval locked (at 1.799996 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "LCD_DE"))
    (pad "77" smd oval locked (at 1.399997 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "NetC12_2"))
    (pad "78" smd oval locked (at 0.999998 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "TV_OUT"))
    (pad "79" smd oval locked (at 0.599998 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "PB7"))
    (pad "80" smd oval locked (at 0.199999 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "PB6"))
    (pad "81" smd oval locked (at -0.2 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "VCC-CORE"))
    (pad "82" smd oval locked (at -0.599999 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "PB5"))
    (pad "83" smd oval locked (at -0.999998 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "VCC3V3"))
    (pad "84" smd oval locked (at -1.399998 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "PB4"))
    (pad "85" smd oval locked (at -1.799997 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "CTP_INT"))
    (pad "86" smd oval locked (at -2.199996 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "CTP_RST"))
    (pad "87" smd oval locked (at -2.599995 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "MICIN3P"))
    (pad "88" smd oval locked (at -2.999994 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "MICIN3N"))
    (pad "89" smd oval locked (at -3.399994 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "AVCC1.8"))
    (pad "90" smd oval locked (at -3.799993 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "NetC78_1"))
    (pad "91" smd oval locked (at -4.199992 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "AGND"))
    (pad "92" smd oval locked (at -4.599991 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "NetC40_2"))
    (pad "93" smd oval locked (at -4.99999 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "94" smd oval locked (at -5.39999 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "95" smd oval locked (at -5.799989 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "LINEINR"))
    (pad "96" smd oval locked (at -6.199988 -7.649998 270) (size 0.18001 1.099998) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "LINEINL"))
    (pad "97" smd oval locked (at -7.649998 -6.199988 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "AVCC1.8"))
    (pad "98" smd oval locked (at -7.649998 -5.799989 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "HPOUTR"))
    (pad "99" smd oval locked (at -7.649998 -5.39999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "HPOUTL"))
    (pad "100" smd oval locked (at -7.649998 -4.99999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "HPOUTFB"))
    (pad "101" smd oval locked (at -7.649998 -4.599991 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "GPADC0"))
    (pad "102" smd oval locked (at -7.649998 -4.199992 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "TP-X1"))
    (pad "103" smd oval locked (at -7.649998 -3.799993 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "TP-X2"))
    (pad "104" smd oval locked (at -7.649998 -3.399994 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "TP-Y1"))
    (pad "105" smd oval locked (at -7.649998 -2.999994 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "TP-Y2"))
    (pad "106" smd oval locked (at -7.649998 -2.599995 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "NetR54_1"))
    (pad "107" smd oval locked (at -7.649998 -2.199996 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "NetC70_1"))
    (pad "108" smd oval locked (at -7.649998 -1.799997 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "TVIN0"))
    (pad "109" smd oval locked (at -7.649998 -1.399998 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "TVIN1"))
    (pad "110" smd oval locked (at -7.649998 -0.999998 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "TVIN_VRP"))
    (pad "111" smd oval locked (at -7.649998 -0.599999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "TVIN_VRN"))
    (pad "112" smd oval locked (at -7.649998 -0.2 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "USB1_P"))
    (pad "113" smd oval locked (at -7.649998 0.199999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "USB1_N"))
    (pad "114" smd oval locked (at -7.649998 0.599998 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "USB0_N"))
    (pad "115" smd oval locked (at -7.649998 0.999998 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "USB0_P"))
    (pad "116" smd oval locked (at -7.649998 1.399997 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "VCC-CORE"))
    (pad "117" smd oval locked (at -7.649998 1.799996 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "VCC-CORE"))
    (pad "118" smd oval locked (at -7.649998 2.199995 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "PG1_SDC1_CMD"))
    (pad "119" smd oval locked (at -7.649998 2.599994 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "PG2_SDC1_D0"))
    (pad "120" smd oval locked (at -7.649998 2.999994 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "NetR39_1"))
    (pad "121" smd oval locked (at -7.649998 3.399993 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "PG3_SDC1_D1"))
    (pad "122" smd oval locked (at -7.649998 3.799992 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "PG5_SDC1_D3"))
    (pad "123" smd oval locked (at -7.649998 4.199991 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "PG4_SDC1_D2"))
    (pad "124" smd oval locked (at -7.649998 4.59999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "WL_REG_ON"))
    (pad "125" smd oval locked (at -7.649998 4.99999 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "AP_WAKE_BT"))
    (pad "126" smd oval locked (at -7.649998 5.399989 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "BT_WAKE_AP"))
    (pad "127" smd oval locked (at -7.649998 5.799988 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "BT_EN"))
    (pad "128" smd oval locked (at -7.649998 6.199987 270) (size 1.099998 0.18001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "VCC3V3"))
    (pad "129" smd rect locked (at 0 0 270) (size 5.720004 5.720004) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 71.678199 126.141603 90)
    (fp_text reference "C71" (at 1.4605 -0.0381 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at -2.9845 -0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "TVIN_VRN") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 83.793999 142.169003 90)
    (fp_text reference "C36" (at 1.536702 -0.1143 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -3.060698 -0.1143 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 60.273599 140.594203 -90)
    (fp_text reference "C50" (at -1.4732 0.0508 unlocked) (layer "F.SilkS") hide)
    (fp_text value "2.2uF" (at 2.9845 0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "NetC50_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 85.292599 127.259203 180)
    (fp_text reference "R17" (at 0.0381 1.5367 unlocked) (layer "F.SilkS") hide)
    (fp_text value "75R" (at 0.0381 -3.0353 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "NetP1_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000003 180) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 158 "LEDA") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 58.470199 138.765403 -90)
    (fp_text reference "C45" (at -1.4732 0.0508 unlocked) (layer "F.SilkS") hide)
    (fp_text value "22pF" (at 2.9845 0.16506 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "32I") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 54.002598 151.707204)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "2" thru_hole circle (at 0 0) (size 5.334 5.334) (drill 2.7) (layers *.Cu *.Mask)
      (net 131 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:LED0402" (layer "F.Cu")
    (tedit 0)
    (at 52.002599 137.207202 -90)
    (fp_text reference "DS2" (at -1.6637 0.1651 unlocked) (layer "F.SilkS") hide)
    (fp_text value "BLUE" (at 3.1877 -0.596654 unlocked) (layer "F.SilkS") hide)
    (pad "A" smd rect (at -0.507997 0) (size 0.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "VCC3V3"))
    (pad "K" smd rect (at 0.507998 0) (size 0.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "NetDS2_K"))
  )
  (footprint "LIB_MANGO.IntLib:MIC-T" locked (layer "F.Cu")
    (tedit 0)
    (at 82.269999 131.450203 -90)
    (fp_text reference "M1" (at -1.8669 -2.8829 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MIC" (at -1.8669 4.4069 -90 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd circle locked (at 0 0 90) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 161 "NetC7_1"))
    (pad "2" smd circle locked (at 0 -1.399999 90) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "NetC7_2"))
    (pad "2" smd circle locked (at 1.4 0 90) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "NetC7_2"))
    (pad "2" smd circle locked (at 0 1.4 90) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "NetC7_2"))
    (pad "2" smd circle locked (at -1.399999 0 90) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "NetC7_2"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 77.774199 126.141603 90)
    (fp_text reference "R3" (at 1.282697 0.0127 unlocked) (layer "F.SilkS") hide)
    (fp_text value "33R" (at -2.8067 0.012702 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000003 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "NetC6_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000003 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 132 "AGND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 68.122199 126.141603 90)
    (fp_text reference "R39" (at 1.452994 -0.057003 unlocked) (layer "F.SilkS") hide)
    (fp_text value "33R" (at -2.9845 -0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000003 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "NetR39_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000003 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "PG0_SDC1_CLK") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 72.668799 126.141603 90)
    (fp_text reference "C69" (at 1.4605 -0.0381 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at -2.9845 -0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "TVIN_VRP") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 76.072399 123.982603)
    (fp_text reference "C85" (at -0.0381 -1.5367 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at -0.0381 3.0353 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "NetC85_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 132 "AGND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "F.Cu")
    (tedit 0)
    (at 54.533199 135.692006)
    (fp_text reference "R6" (at -0.2667 -1.0795 unlocked) (layer "F.SilkS") hide)
    (fp_text value "5.1K" (at -0.2667 2.6035 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 -0.000003) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 130 "NetDS1_K") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 -0.000003) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "F.Cu")
    (tedit 0)
    (at 61.315001 139.679803 90)
    (fp_text reference "C44" (at 1.4732 -0.0508 unlocked) (layer "F.SilkS") hide)
    (fp_text value "2.2uF" (at -2.9845 -0.0381 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "LDOA-OUT") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 61.467399 150.586604 90)
    (fp_text reference "C64" (at 1.4732 0.0508 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "AVDD2V8") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 55 "AAGND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 58.571796 148.468203)
    (fp_text reference "R12" (at 1.5367 0.1143 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "75K 1%" (at -3.3147 0.1143 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 117 "VCC-CORE") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 122 "NetR12_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 73.405399 138.968603 90)
    (fp_text reference "R76" (at 1.5367 0.0381 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at -3.0353 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 156 "SPI0_MISO") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 77.469399 129.723003 -90)
    (fp_text reference "C40" (at 1.282698 -0.0127 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.47uF" (at -2.8067 -0.012702 180 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 132 "AGND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "NetC40_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 55.599999 126.649603 -90)
    (fp_text reference "R28" (at -1.026398 -0.474698 unlocked) (layer "B.SilkS") hide)
    (fp_text value "5.1K" (at 3.409496 -0.4631 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 78 "NetJ3_A5") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 56.920799 144.836003 180)
    (fp_text reference "R2" (at -1.8923 -1.257298 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100K" (at -1.8923 2.781297 180 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "NetC4_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 76.326399 133.964803)
    (fp_text reference "C2" (at -1.7653 -1.2573 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at -5.8293 2.7813 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 76.859799 126.141603 90)
    (fp_text reference "R64" (at 1.4605 0.0381 unlocked) (layer "B.SilkS") hide)
    (fp_text value "33R" (at -2.9845 -0.723654 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "NetC80_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 132 "AGND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:VLS2016" (layer "B.Cu")
    (tedit 0)
    (at 62.153199 143.2248 -90)
    (fp_text reference "L1" (at 0.248806 -0.285602 unlocked) (layer "B.SilkS") hide)
    (fp_text value "2.2uH" (at -4.1699 0.740098 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect (at 0.675 0 180) (size 1.6 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 129 "NetL1_1"))
    (pad "2" smd rect (at -0.675 0 180) (size 1.6 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "VCC3V3"))
  )
  (footprint "LIB_MANGO.IntLib:MINISW" locked (layer "B.Cu")
    (tedit 0)
    (at 52.002599 126.707203 -90)
    (fp_text reference "S1" (at 3.5941 1.2573 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "SW-CE" (at -5.0927 1.2573 180 unlocked) (layer "B.SilkS") hide)
    (pad "0" smd rect locked (at 2.3 0 270) (size 1 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "0" smd rect locked (at -2.300001 0 270) (size 1 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "1" smd rect locked (at -1.675001 -1.55 270) (size 1.15 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "2" smd rect locked (at 1.675 -1.55 90) (size 1.15 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 157 "SPI0_MOSI"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 78.637799 125.913003 -90)
    (fp_text reference "R20" (at -1.5367 -0.0381 unlocked) (layer "B.SilkS") hide)
    (fp_text value "150K 1%" (at 3.2893 -0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "NetR20_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "NetC54_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 55.701596 144.861403 90)
    (fp_text reference "C76" (at 1.4605 0.0381 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 125 "VCCIN") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 82.066799 129.545203 90)
    (fp_text reference "R34" (at 1.4605 0.0381 unlocked) (layer "B.SilkS") hide)
    (fp_text value "1K" (at -2.9845 -0.850613 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "NetC7_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 132 "AGND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 82.498599 127.818003 180)
    (fp_text reference "R36" (at 0.158603 -1.010806 unlocked) (layer "B.SilkS") hide)
    (fp_text value "5.1K" (at 0.5715 -5.0673 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 81 "LCD_PWM") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 85.267199 125.532003 -90)
    (fp_text reference "R4" (at -0.520697 1.1303 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "2R7" (at -0.520697 -2.6543 90 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 159 "LEDK") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 73.024399 143.362803 180)
    (fp_text reference "C77" (at -0.476179 1.023488 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -0.4699 -3.4163 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 120 "LDOA-OUT") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 77.164599 147.579203 90)
    (fp_text reference "R35" (at 1.505869 0.147962 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at -2.951831 0.135262 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "NetR35_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:WSON-SPIFLASH" locked (layer "B.Cu")
    (tedit 0)
    (at 69.290599 135.717403 90)
    (fp_text reference "U3" (at -0.571503 -3.289298 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "SPIFLASH_SOP8W" (at -17.310103 5.2451 90 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd oval locked (at -3.764001 1.905) (size 0.45 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 155 "SPI0_CS"))
    (pad "2" smd oval locked (at -3.764001 0.635) (size 0.45 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 156 "SPI0_MISO"))
    (pad "3" smd oval locked (at -3.764001 -0.635) (size 0.45 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 106 "SPI0_WP"))
    (pad "4" smd rect locked (at 0 0 90) (size 3.4 4.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "4" smd oval locked (at -3.764001 -1.905) (size 0.45 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "5" smd oval locked (at 3.764 -1.905) (size 0.45 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 157 "SPI0_MOSI"))
    (pad "6" smd oval locked (at 3.764 -0.635) (size 0.45 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 154 "SPI0_CLK"))
    (pad "7" smd oval locked (at 3.764 0.635) (size 0.45 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 107 "SPI0_HOLD"))
    (pad "8" smd oval locked (at 3.764 1.905) (size 0.45 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "VCC3V3"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 57.098599 149.154003 180)
    (fp_text reference "C65" (at -0.0508 1.4732 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -0.0381 -2.9845 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 85.013199 128.275203 -90)
    (fp_text reference "C59" (at -1.2827 4.0767 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 2.806703 3.8227 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 70.382799 142.067403 -90)
    (fp_text reference "C52" (at -1.4732 -0.0508 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at 2.9845 -0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 116 "VCC-DRAM") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 72.871999 132.415403 90)
    (fp_text reference "C42" (at 1.071994 3.625997 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 72.160799 130.535803 -90)
    (fp_text reference "R54" (at -1.4732 -0.0508 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC/1K" (at 2.9845 -0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "NetR54_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:TEST-POINT" (layer "B.Cu")
    (tedit 0)
    (at 68.833399 141.584803 90)
    (fp_text reference "TP4" (at 1.2319 0.2413 unlocked) (layer "B.SilkS") hide)
    (fp_text value "TEST POINT" (at -2.7559 0.2413 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd circle (at 0 0 90) (size 0.762 0.762) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND") (solder_paste_margin -0.4))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 79.831599 129.545203 90)
    (fp_text reference "R55" (at 0.521756 -0.864388 unlocked) (layer "B.SilkS") hide)
    (fp_text value "75R" (at -3.4925 0.2921 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 35 "AVCC1.8") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "NetC81_1") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 65.556799 147.604603 90)
    (fp_text reference "R53" (at 1.4732 0.0508 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0R" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 55 "AAGND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "D:_×ÊÁÏ¿â_ADLIB_A.PcbLib_AP6212" locked (layer "B.Cu")
    (tedit 0)
    (at 67.0026 122.307204)
    (fp_text reference "U6" (at 6.140597 -7.167994 unlocked) (layer "B.SilkS") hide)
    (fp_text value "WIFI" (at -2.412221 0 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd oval locked (at -5.699999 4.499999 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "2" smd oval locked (at -5.699999 3.599998 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 63 "NetC58_2"))
    (pad "3" smd oval locked (at -5.699999 2.699997 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "4" smd oval locked (at -5.699999 1.799999 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "5" smd oval locked (at -5.699999 0.900001 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "6" smd oval locked (at -5.699999 0 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 70 "AP_WAKE_BT"))
    (pad "7" smd oval locked (at -5.699999 -0.900001 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 68 "BT_WAKE_AP"))
    (pad "8" smd oval locked (at -5.699999 -1.799999 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "9" smd oval locked (at -5.699999 -2.699997 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 85 "VCC_WIFI"))
    (pad "10" smd oval locked (at -5.699999 -3.599998 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "11" smd oval locked (at -5.699999 -4.499999 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "12" smd oval locked (at -4.499999 -5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 58 "WL_REG_ON"))
    (pad "13" smd oval locked (at -3.599998 -5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "WL_WAKE_AP"))
    (pad "14" smd oval locked (at -2.699997 -5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 91 "PG4_SDC1_D2"))
    (pad "15" smd oval locked (at -1.799999 -5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 90 "PG5_SDC1_D3"))
    (pad "16" smd oval locked (at -0.900001 -5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 94 "PG1_SDC1_CMD"))
    (pad "17" smd oval locked (at 0 -5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 95 "PG0_SDC1_CLK"))
    (pad "18" smd oval locked (at 0.9 -5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 93 "PG2_SDC1_D0"))
    (pad "19" smd oval locked (at 1.799999 -5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 92 "PG3_SDC1_D1"))
    (pad "20" smd oval locked (at 2.699997 -5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "21" smd oval locked (at 3.599998 -5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "22" smd oval locked (at 4.499998 -5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "VCC3V3"))
    (pad "23" smd oval locked (at 5.699998 -4.499999 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "24" smd oval locked (at 5.699998 -3.599998 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "NetR47_1"))
    (pad "25" smd oval locked (at 5.699998 -2.699997 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "26" smd oval locked (at 5.699998 -1.799999 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "27" smd oval locked (at 5.699998 -0.900001 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "28" smd oval locked (at 5.699998 0 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "29" smd oval locked (at 5.699998 0.900001 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "30" smd oval locked (at 5.699998 1.799999 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 96 "NetR41_2"))
    (pad "31" smd oval locked (at 5.699998 2.699997 90) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "32" smd oval locked (at 5.699998 3.599998 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "33" smd oval locked (at 5.699998 4.499999 270) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "34" smd oval locked (at 4.499998 5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 69 "BT_EN"))
    (pad "35" smd oval locked (at 3.599998 5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "36" smd oval locked (at 2.699997 5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "37" smd oval locked (at 1.799999 5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "38" smd oval locked (at 0.9 5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "39" smd oval locked (at 0 5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "40" smd oval locked (at -0.900001 5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "41" smd oval locked (at -1.799999 5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 89 "UART1_CTS"))
    (pad "42" smd oval locked (at -2.699997 5.699999) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "UART1_RX"))
    (pad "43" smd oval locked (at -3.599998 5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "UART1_TX"))
    (pad "44" smd oval locked (at -4.499999 5.699999 180) (size 0.5 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 88 "UART1_RTS"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 68.503199 130.612003)
    (fp_text reference "R49" (at 2.034776 2.309965 unlocked) (layer "B.SilkS") hide)
    (fp_text value "33R" (at -0.386901 2.559505 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 110 "NetR49_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 154 "SPI0_CLK") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 74.904001 117.073803 90)
    (fp_text reference "C19" (at -0.241206 0.600596 unlocked) (layer "B.SilkS") hide)
    (fp_text value "1uF" (at -2.008902 5.418105 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 80.695199 127.818003)
    (fp_text reference "R32" (at 1.536697 0.1143 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at -3.0607 0.1143 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "PD22") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 81 "LCD_PWM") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 81.990599 132.339203 -135)
    (fp_text reference "C46" (at 1.5367 0.1143 135 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -3.060699 0.1143 135 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.457198 0 225) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 161 "NetC7_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 225) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "MICIN3P") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.01740048367 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 69.6026 143.306398 90)
    (fp_text reference "C38" (at 1.282698 -0.0127 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -2.8067 -0.012703 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 117 "VCC-CORE") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 82.549399 130.866003 180)
    (fp_text reference "C7" (at -0.4953 1.0795 unlocked) (layer "B.SilkS") hide)
    (fp_text value "100pF" (at -2.018807 -2.324182 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 161 "NetC7_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "NetC7_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 60.629199 143.007203 90)
    (fp_text reference "C29" (at 1.5367 0.1143 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -3.0607 0.1143 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 56.920799 127.868806 180)
    (fp_text reference "R78" (at -0.0381 1.5367 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at -0.0381 -3.0353 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 157 "SPI0_MOSI") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 78.409199 129.723003 -90)
    (fp_text reference "R15" (at 1.5367 0.1143 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0R" (at -3.0607 0.1143 180 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 132 "AGND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 71.144799 143.388203)
    (fp_text reference "C24" (at 1.282697 -0.0127 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "1uF" (at -2.8067 -0.012702 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 116 "VCC-DRAM") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 54.685599 128.326003 90)
    (fp_text reference "C82" (at 7.390099 5.957308 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at 2.945099 5.957308 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 125 "VCCIN") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 59.663999 125.913003 180)
    (fp_text reference "R38" (at -0.438002 1.071994 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0R" (at -0.6477 -3.1369 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 63 "NetC58_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 64 "NetC48_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 60.121199 122.661803 -90)
    (fp_text reference "R46" (at -1.048199 0.374206 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC/100K" (at 3.409501 -3.294903 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 70 "AP_WAKE_BT") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:TEST-POINT" (layer "B.Cu")
    (tedit 0)
    (at 75.914881 125.684403 90)
    (fp_text reference "TP10" (at 1.2319 0.2413 unlocked) (layer "B.SilkS") hide)
    (fp_text value "TEST POINT" (at -2.7559 0.2413 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd circle (at 0 0 90) (size 0.762 0.762) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 132 "AGND") (solder_paste_margin -0.4))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 58.266999 119.156603 90)
    (fp_text reference "R58" (at 1.473205 -0.8128 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0R" (at -2.984495 -0.8255 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 85 "VCC_WIFI") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:MINISW" locked (layer "B.Cu")
    (tedit 0)
    (at 52.002599 144.707202 -90)
    (fp_text reference "S2" (at 3.5941 1.2573 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "SW-CE" (at -5.0927 1.2573 180 unlocked) (layer "B.SilkS") hide)
    (pad "0" smd rect locked (at 2.300001 0 270) (size 1 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "0" smd rect locked (at -2.3 0 270) (size 1 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "1" smd rect locked (at -1.675 -1.55 270) (size 1.15 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 109 "RESET"))
    (pad "2" smd rect locked (at 1.675001 -1.55 90) (size 1.15 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:TEST-POINT" (layer "B.Cu")
    (tedit 0)
    (at 78.764799 123.550803 90)
    (fp_text reference "TP9" (at 1.2319 0.2413 unlocked) (layer "B.SilkS") hide)
    (fp_text value "TEST POINT" (at -2.7559 0.2413 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd circle (at 0 0 90) (size 0.762 0.762) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "NetC15_2") (solder_paste_margin -0.4))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 65.505999 143.464403 180)
    (fp_text reference "C66" (at -0.0508 1.4732 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -0.0381 -2.9845 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "VCC-RMII-CSI") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 63.677199 143.007203 -90)
    (fp_text reference "C28" (at 1.5367 0.1143 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -3.0607 0.1143 180 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 78.26102 147.579203 90)
    (fp_text reference "R72" (at 1.478394 0.057003 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "DVP_SCL") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "VCC-RMII-CSI") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:TEST-POINT" (layer "B.Cu")
    (tedit 0)
    (at 65.607599 137.546203 90)
    (fp_text reference "TP3" (at 1.2319 0.2413 unlocked) (layer "B.SilkS") hide)
    (fp_text value "TEST POINT" (at -2.7559 0.2413 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd circle (at 0 0 90) (size 0.762 0.762) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "VCC_RTC") (solder_paste_margin -0.4))
  )
  (footprint "LIB_MANGO.IntLib:FFC{slash}SM0.5-1H40" locked (layer "B.Cu")
    (tedit 0)
    (at 88.002598 135.707203 -90)
    (fp_text reference "P1" (at 24.5745 1.9685 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "FFC40-RGBLCD" (at -3.2385 1.9685 180 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect locked (at -9.749986 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 159 "LEDK"))
    (pad "2" smd rect locked (at -9.249987 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "NetP1_2"))
    (pad "3" smd rect locked (at -8.749988 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "4" smd rect locked (at -8.249989 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "VCC3V3"))
    (pad "5" smd rect locked (at -7.74999 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "6" smd rect locked (at -7.249991 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "7" smd rect locked (at -6.749992 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "LCD_D18"))
    (pad "8" smd rect locked (at -6.249993 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 140 "LCD_D19"))
    (pad "9" smd rect locked (at -5.749994 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 141 "LCD_D20"))
    (pad "10" smd rect locked (at -5.249995 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "LCD_D21"))
    (pad "11" smd rect locked (at -4.749996 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 143 "LCD_D22"))
    (pad "12" smd rect locked (at -4.249997 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 144 "LCD_D23"))
    (pad "13" smd rect locked (at -3.749998 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "14" smd rect locked (at -3.249999 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "15" smd rect locked (at -2.75 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 134 "LCD_D10"))
    (pad "16" smd rect locked (at -2.250001 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 135 "LCD_D11"))
    (pad "17" smd rect locked (at -1.750002 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 136 "LCD_D12"))
    (pad "18" smd rect locked (at -1.250003 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 137 "LCD_D13"))
    (pad "19" smd rect locked (at -0.750004 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 138 "LCD_D14"))
    (pad "20" smd rect locked (at -0.250005 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 139 "LCD_D15"))
    (pad "21" smd rect locked (at 0.249994 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "22" smd rect locked (at 0.749993 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "23" smd rect locked (at 1.249992 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 73 "D0_P"))
    (pad "24" smd rect locked (at 1.749991 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 74 "D0_N"))
    (pad "25" smd rect locked (at 2.24999 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 71 "D1_P"))
    (pad "26" smd rect locked (at 2.749989 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 72 "D1_N"))
    (pad "27" smd rect locked (at 3.249988 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "CK_P"))
    (pad "28" smd rect locked (at 3.749987 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 76 "CK_N"))
    (pad "29" smd rect locked (at 4.249986 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "30" smd rect locked (at 4.749985 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "LCD_CLK"))
    (pad "31" smd rect locked (at 5.249984 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "VCC3V3"))
    (pad "32" smd rect locked (at 5.749983 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 146 "LCD_HSYNC"))
    (pad "33" smd rect locked (at 6.249982 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 147 "LCD_VSYNC"))
    (pad "34" smd rect locked (at 6.749981 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 145 "LCD_DE"))
    (pad "35" smd rect locked (at 7.24998 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "VCC3V3"))
    (pad "36" smd rect locked (at 7.749979 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "37" smd rect locked (at 8.249978 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 105 "TP-X1"))
    (pad "38" smd rect locked (at 8.749977 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 103 "TP-Y1"))
    (pad "39" smd rect locked (at 9.249976 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 104 "TP-X2"))
    (pad "40" smd rect locked (at 9.749975 1.405102 180) (size 0.65 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 102 "TP-Y2"))
    (pad "G" smd rect locked (at -10.634998 -1.405098 180) (size 1.15 0.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "G" smd rect locked (at 10.635003 -1.405098 180) (size 1.15 0.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 78.637796 127.614803 90)
    (fp_text reference "C54" (at 1.5367 0.0381 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -3.0353 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 113 "HPOUTL") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "NetC54_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 55.599994 128.326003 90)
    (fp_text reference "R30" (at 1.451394 0.049697 unlocked) (layer "B.SilkS") hide)
    (fp_text value "5.1K" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "NetJ3_B5") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 58.597199 144.759803 180)
    (fp_text reference "C33" (at 1.5367 0.1143 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -3.0607 0.1143 90 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 117 "VCC-CORE") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:VLS2016" (layer "B.Cu")
    (tedit 0)
    (at 62.076999 146.410803 90)
    (fp_text reference "L3" (at -0.8509 1.7145 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "2.2uH" (at -0.8509 -3.2385 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect (at 0.675 0) (size 1.6 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 127 "NetL3_1"))
    (pad "2" smd rect (at -0.675 0) (size 1.6 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 116 "VCC-DRAM"))
  )
  (footprint "LIB_MANGO.IntLib:SOT23" locked (layer "B.Cu")
    (tedit 0)
    (at 59.206799 153.776803 -90)
    (fp_text reference "U8" (at -2.5146 -1.2446 unlocked) (layer "B.SilkS") hide)
    (fp_text value "XC6206-1.2" (at 4.0259 -7.09741 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect locked (at -0.949998 -1.174996 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "2" smd rect locked (at 0.950001 -1.175001 270) (size 0.899998 0.950011) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "DVP_DVDD"))
    (pad "3" smd rect locked (at 0.000003 1.175004 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "VCC3V3"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 83.057399 129.545203 -90)
    (fp_text reference "R27" (at 1.5367 0.1143 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "1K" (at -3.060702 0.1143 180 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "NetC81_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 161 "NetC7_1") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 74.268999 138.359003 -90)
    (fp_text reference "R75" (at -1.5367 -0.0381 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at 3.0353 -0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 156 "SPI0_MISO") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:SOT23" (layer "B.Cu")
    (tedit 0)
    (at 59.200202 150.586601 -90)
    (fp_text reference "U9" (at -2.064593 -1.694592 unlocked) (layer "B.SilkS") hide)
    (fp_text value "XC6206-2.8" (at 4.475907 -1.707292 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect (at -0.949998 -1.174997 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 55 "AAGND"))
    (pad "2" smd rect (at 0.950001 -1.175002 270) (size 0.899998 0.950011) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 54 "AVDD2V8"))
    (pad "3" smd rect (at 0.000003 1.175004 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "VCC3V3"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 58.749599 125.176403)
    (fp_text reference "C48" (at 0.044597 -1.452997 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at 0.0381 2.9845 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 64 "NetC48_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 83.565399 122.941203 180)
    (fp_text reference "R81" (at -0.0381 1.5367 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at -0.0381 -3.0353 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "CTP_RST") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 76.252604 147.579203 90)
    (fp_text reference "R50" (at 1.262258 -1.465234 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at -3.195442 -1.477934 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 37 "NetR50_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:FFC{slash}SM0.5-2H24-OV5640" locked (layer "B.Cu")
    (tedit 0)
    (at 71.002599 151.207202 180)
    (fp_text reference "U7" (at -1.421989 -1.879354 unlocked) (layer "B.SilkS") hide)
    (fp_text value "OV-DVP" (at -1.977126 -5.559725 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect locked (at 5.74997 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "2" smd rect locked (at 5.249971 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 55 "AAGND"))
    (pad "3" smd rect locked (at 4.749972 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "DVP_SDA"))
    (pad "4" smd rect locked (at 4.249973 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 54 "AVDD2V8"))
    (pad "5" smd rect locked (at 3.749974 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "DVP_SCL"))
    (pad "6" smd rect locked (at 3.249975 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "DVP_RST"))
    (pad "7" smd rect locked (at 2.749976 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "DVP_VSYNC"))
    (pad "8" smd rect locked (at 2.249977 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "9" smd rect locked (at 1.749978 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "DVP_HSYNC"))
    (pad "10" smd rect locked (at 1.249979 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "DVP_DVDD"))
    (pad "11" smd rect locked (at 0.74998 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "VCC-RMII-CSI"))
    (pad "12" smd rect locked (at 0.249981 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 46 "DVP-Y9"))
    (pad "13" smd rect locked (at -0.250018 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "DVP_XCLK"))
    (pad "14" smd rect locked (at -0.750017 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "DVP-Y8"))
    (pad "15" smd rect locked (at -1.250016 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "16" smd rect locked (at -1.750015 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "DVP-Y7"))
    (pad "17" smd rect locked (at -2.250014 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "DVP_PCLK"))
    (pad "18" smd rect locked (at -2.750013 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 49 "DVP-Y6"))
    (pad "19" smd rect locked (at -3.250012 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 53 "DVP-Y2"))
    (pad "20" smd rect locked (at -3.750011 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 50 "DVP-Y5"))
    (pad "21" smd rect locked (at -4.25001 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 52 "DVP-Y3"))
    (pad "22" smd rect locked (at -4.750009 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 51 "DVP-Y4"))
    (pad "23" smd rect locked (at -5.250008 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "NetR50_1"))
    (pad "24" smd rect locked (at -5.750007 1.625 270) (size 1.3 0.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "NetR35_1"))
    (pad "P0" smd rect locked (at 7.649984 -1.625001 270) (size 2.2 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "P0" smd rect locked (at -7.649985 -1.625001 270) (size 2.2 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 71.601999 142.067403 -90)
    (fp_text reference "C21" (at -4.872799 5.982198 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -1.558099 6.129902 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 116 "VCC-DRAM") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 60.095799 119.156603 -90)
    (fp_text reference "C14" (at -1.7907 3.822703 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at 3.3147 6.362703 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 85 "VCC_WIFI") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 59.740199 143.007203 -90)
    (fp_text reference "C25" (at 1.5367 0.1143 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -3.0607 0.1143 180 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 125 "VCCIN") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 79.221999 147.579203 90)
    (fp_text reference "R73" (at 1.478394 0.057002 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "DVP_SDA") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "VCC-RMII-CSI") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 81.533399 122.941203)
    (fp_text reference "C51" (at 1.5367 0.1143 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -3.0607 0.1143 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 74.014999 117.073803 90)
    (fp_text reference "R47" (at 1.452994 0.044597 unlocked) (layer "B.SilkS") hide)
    (fp_text value "47K" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "NetR47_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 66.521999 141.584803 180)
    (fp_text reference "R74" (at 0.062492 1.624297 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at 0.062492 -2.820703 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 120 "LDOA-OUT") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 109 "RESET") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 68.402605 143.3064 90)
    (fp_text reference "R42" (at 1.452994 0.057002 unlocked) (layer "B.SilkS") hide)
    (fp_text value "240R 1%" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 121 "NetR42_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 71.043199 129.240403 180)
    (fp_text reference "R37" (at -0.0508 1.4732 unlocked) (layer "B.SilkS") hide)
    (fp_text value "100K" (at 2.247161 -2.9845 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 69 "BT_EN") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 66.521999 140.746603)
    (fp_text reference "R7" (at 1.282697 -0.0127 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at -2.8067 -0.012702 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 155 "SPI0_CS") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:FPC6" locked (layer "B.Cu")
    (tedit 0)
    (at 80.999999 119.385203 180)
    (fp_text reference "P4" (at 0.5842 0.330197 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "FPC6" (at 30.2641 7.9883 270 unlocked) (layer "F.SilkS") hide)
    (pad "0" smd rect locked (at -3.300001 1.383792) (size 1.6 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "0" smd rect locked (at 3.300001 1.391874) (size 1.6 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "1" smd rect locked (at -1.25002 -1.391875 180) (size 0.249987 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "CTP_RST"))
    (pad "2" smd oval locked (at -0.750021 -1.391875 180) (size 0.249987 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "VCC3V3"))
    (pad "3" smd oval locked (at -0.250022 -1.391875 180) (size 0.249987 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "4" smd oval locked (at 0.249977 -1.391875 180) (size 0.249987 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 57 "CTP_INT"))
    (pad "5" smd oval locked (at 0.749976 -1.391875 180) (size 0.249987 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "DVP_SDA"))
    (pad "6" smd oval locked (at 1.249975 -1.391875 180) (size 0.249987 2.799994) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "DVP_SCL"))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 56.920799 143.058003)
    (fp_text reference "R23" (at -0.8763 -1.536695 unlocked) (layer "B.SilkS") hide)
    (fp_text value "100K" (at -0.8763 3.035305 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.457197 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "NetR23_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 81.380999 131.907403 -135)
    (fp_text reference "C47" (at -1.05967 1.005789 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at 1.095911 -3.12481 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.457198 0 225) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "NetC7_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 225) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "MICIN3N") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.01740048367 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 54.685599 126.649603 -90)
    (fp_text reference "C83" (at -1.522697 -0.089908 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at 2.922303 -0.089908 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 125 "VCCIN") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 61.467399 153.776806 -90)
    (fp_text reference "C62" (at -1.4732 -0.0508 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at 2.9845 -0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "DVP_DVDD") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 68.757199 129.240403)
    (fp_text reference "C39" (at 1.282697 -0.0127 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -2.8067 -0.012702 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 117 "VCC-CORE") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:SOT23-6" locked (layer "B.Cu")
    (tedit 0)
    (at 82.711199 125.694604 180)
    (fp_text reference "U5" (at -0.952508 -2.5527 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MT9284-28J" (at -6.794503 4.3053 180 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect locked (at -1.000001 0.950001 90) (size 0.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 160 "NetD1_A"))
    (pad "2" smd rect locked (at -1.000001 0 90) (size 0.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "3" smd rect locked (at -1.000001 -0.949998 90) (size 0.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 159 "LEDK"))
    (pad "4" smd rect locked (at 1 -0.949998 90) (size 0.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "LCD_PWM"))
    (pad "5" smd rect locked (at 1 0 90) (size 0.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 158 "LEDA"))
    (pad "6" smd rect locked (at 1 0.950001 90) (size 0.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 125 "VCCIN"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 69.747799 147.579203 90)
    (fp_text reference "C67" (at 1.452994 0.057002 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "DVP_DVDD") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 54.838001 146.207603 90)
    (fp_text reference "R26" (at 2.024545 -0.686044 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "5.1K" (at -3.176303 -0.164091 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 79 "NetJ2_B5") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 74.192799 128.046603 -90)
    (fp_text reference "R71" (at -0.927105 -1.880654 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0R" (at 2.984505 -0.9017 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "NetC70_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 35 "AVCC1.8") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 76.326399 134.955403)
    (fp_text reference "C53" (at 0.0508 -1.4732 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at 0.0381 2.9845 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 117 "VCC-CORE") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 76.504199 128.046603 90)
    (fp_text reference "C80" (at 1.035499 0.4631 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -3.409501 0.4631 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 113 "HPOUTL") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "NetC80_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 78.409199 131.399403 90)
    (fp_text reference "C78" (at 1.4605 0.0381 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.47uF" (at -2.9845 0.672894 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "NetC78_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 132 "AGND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 75.284999 128.046603 -90)
    (fp_text reference "C22" (at -1.7907 3.8227 unlocked) (layer "F.SilkS") hide)
    (fp_text value "2.2uF" (at 3.3147 6.3627 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 132 "AGND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 35 "AVCC1.8") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 60.248199 148.468203 180)
    (fp_text reference "R13" (at 1.5367 0.1143 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "150K 1%" (at -3.3147 0.1143 90 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 122 "NetR12_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 80.237999 125.709803 -90)
    (fp_text reference "C23" (at -1.5367 3.949705 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at 3.0607 5.219708 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 125 "VCCIN") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 68.223799 140.746603 180)
    (fp_text reference "R33" (at 0.812551 -5.155545 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at -0.0381 -2.9845 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 106 "SPI0_WP") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 77.774196 126.141603 -90)
    (fp_text reference "C5" (at -1.7653 -1.2573 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -5.8293 2.7813 -90 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 132 "AGND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 35 "AVCC1.8") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:TEST-POINT" (layer "B.Cu")
    (tedit 0)
    (at 74.573799 125.684403 90)
    (fp_text reference "TP11" (at 1.2319 0.2413 unlocked) (layer "B.SilkS") hide)
    (fp_text value "TEST POINT" (at -2.7559 0.2413 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd circle (at 0 0 90) (size 0.762 0.762) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "TVIN0") (solder_paste_margin -0.4))
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 56.920799 143.947003)
    (fp_text reference "R1" (at -1.384298 -1.2573 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100K" (at -1.8923 2.781298 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "NetC4_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 65.988599 145.013803 -90)
    (fp_text reference "R56" (at -1.0668 -0.4572 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0R" (at 2.5781 -0.4445 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "VCC-RMII-CSI") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "AVDD2V8") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 76.326399 137.901803 180)
    (fp_text reference "R79" (at 0.8128 1.473205 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0R" (at 0.8255 -2.984495 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "NetC12_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 55.701599 142.956403 -90)
    (fp_text reference "R24" (at -1.453652 0.577751 -90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "5.1K" (at -2.691102 -6.553304 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 80 "NetJ2_A5") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 56.920799 128.783206)
    (fp_text reference "R77" (at 0.0381 -1.5367 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at 0.0381 3.0353 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 157 "SPI0_MOSI") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 76.326399 135.946003)
    (fp_text reference "R60" (at 0.057002 -1.452994 unlocked) (layer "B.SilkS") hide)
    (fp_text value "75R" (at 0.0381 2.9845 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "TV_OUT") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 60.095799 124.719203 -90)
    (fp_text reference "C58" (at -0.757052 1.327661 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at 2.9845 1.993242 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 63 "NetC58_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 74.472199 118.597803 180)
    (fp_text reference "R84" (at -0.0381 1.5367 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at 1.358448 -3.0353 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 56 "PG11") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "NetR47_1") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 65.074199 145.013803 90)
    (fp_text reference "R57" (at 1.071994 0.438002 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at -2.5781 0.4445 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "VCC-RMII-CSI") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 67.385599 147.604603 90)
    (fp_text reference "R52" (at 1.4732 0.0508 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at -2.9845 0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "DVP_RST") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 109 "RESET") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 77.469401 131.399403 90)
    (fp_text reference "C11" (at 1.5367 0.1143 unlocked) (layer "B.SilkS") hide)
    (fp_text value "2.2uF" (at -3.0607 0.1143 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 35 "AVCC1.8") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 132 "AGND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 72.821199 142.067403 -90)
    (fp_text reference "C37" (at -1.15998 0.687421 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at 3.28502 0.687421 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 117 "VCC-CORE") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:VLS2016" (layer "B.Cu")
    (tedit 0)
    (at 58.800399 146.207603)
    (fp_text reference "L2" (at -0.8509 1.714503 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "2.2uH" (at -0.8509 -3.238502 180 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect (at 0.675 0 270) (size 1.6 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "NetL2_1"))
    (pad "2" smd rect (at -0.675 0 270) (size 1.6 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 117 "VCC-CORE"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 83.920999 128.275203 90)
    (fp_text reference "C60" (at -1.5367 3.949705 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at 3.0607 5.219707 180 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 70.585999 130.612003 180)
    (fp_text reference "R25" (at 1.5367 0.1143 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at -3.0607 0.1143 90 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 107 "SPI0_HOLD") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:SOT23-6" locked (layer "B.Cu")
    (tedit 0)
    (at 76.072399 123.322203 180)
    (fp_text reference "U10" (at -2.212998 2.788996 unlocked) (layer "B.SilkS") hide)
    (fp_text value "PAM8301" (at -1.5875 -4.0767 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect locked (at -1 0.95 90) (size 0.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "NetP6_1"))
    (pad "2" smd rect locked (at -1 0.000002 90) (size 0.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 132 "AGND"))
    (pad "3" smd rect locked (at -1 -0.949998 90) (size 0.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "NetR20_1"))
    (pad "4" smd rect locked (at 1.000001 -0.949998 90) (size 0.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "NetC85_1"))
    (pad "5" smd rect locked (at 1.000001 0 90) (size 0.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "NetC85_1"))
    (pad "6" smd rect locked (at 1.000001 0.95 90) (size 0.55 1.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "NetP6_2"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 54.837999 143.464403 -90)
    (fp_text reference "C84" (at -7.491697 -5.804908 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at -3.046697 -5.804908 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 109 "RESET") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 58.597199 147.579203)
    (fp_text reference "C32" (at 1.5367 0.1143 270 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10uF" (at -3.0607 0.1143 270 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 117 "VCC-CORE") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:SOT23" locked (layer "B.Cu")
    (tedit 0)
    (at 74.954799 130.561203 -90)
    (fp_text reference "U2" (at -1.2827 -2.5019 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "XC6206-1.8V" (at -7.3787 4.0259 -90 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect locked (at -0.949998 -1.174996 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 132 "AGND"))
    (pad "2" smd rect locked (at 0.950001 -1.175001 270) (size 0.899998 0.950011) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "AVCC1.8"))
    (pad "3" smd rect locked (at 0.000003 1.175004 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "VCC3V3"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 56.920799 145.750403)
    (fp_text reference "C4" (at -1.7653 -1.2573 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at -5.8293 2.7813 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "NetC4_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 70.662199 147.579203 -90)
    (fp_text reference "C61" (at -1.8982 -0.4758 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at 2.5595 -0.4631 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 55 "AAGND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "VCC-RMII-CSI") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 59.181399 119.156603 -90)
    (fp_text reference "C16" (at -1.7907 3.568698 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 3.3147 6.3627 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 85 "VCC_WIFI") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 66.471199 147.604603 -90)
    (fp_text reference "C63" (at -1.4732 -0.0508 unlocked) (layer "B.SilkS") hide)
    (fp_text value "0.1uF" (at 2.9845 -0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 55 "AAGND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "AVDD2V8") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:TEST-POINT" (layer "B.Cu")
    (tedit 0)
    (at 79.425199 127.614803 90)
    (fp_text reference "TP8" (at 1.2319 0.2413 unlocked) (layer "B.SilkS") hide)
    (fp_text value "TEST POINT" (at -2.7559 0.2413 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd circle (at 0 0 90) (size 0.762 0.762) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "NetC54_2") (solder_paste_margin -0.4))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 80.923799 129.545203 -90)
    (fp_text reference "C81" (at -1.244844 3.326824 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at 2.9845 -0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "NetC81_1") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 132 "AGND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:TFCARD-1040310811" locked (layer "B.Cu")
    (tedit 0)
    (at 53.502599 135.707203 90)
    (fp_text reference "J1" (at 0.3048 0.2286 180 unlocked) (layer "B.SilkS") hide)
    (fp_text value "TF5033981892" (at -8.3947 2.705097 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd rect locked (at 3.105 0.239499 90) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 152 "SDC0_D2"))
    (pad "2" smd rect locked (at 2.005 0.239499 90) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 153 "SDC0_D3"))
    (pad "3" smd rect locked (at 0.905 0.239499 90) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 149 "SDC0_CMD"))
    (pad "4" smd rect locked (at -0.195001 0.239499 90) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "VCC3V3"))
    (pad "5" smd rect locked (at -1.295001 0.239499 90) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 148 "SDC0_CLK"))
    (pad "6" smd rect locked (at -2.394999 0.239499 90) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "7" smd rect locked (at -3.494999 0.239499 90) (size 0.85 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 150 "SDC0_D0"))
    (pad "8" smd rect locked (at -4.544999 0.239499 90) (size 0.75 1.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 151 "SDC0_D1"))
    (pad "G1" smd rect locked (at 5.565001 0.3645 90) (size 1.55 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "G2" smd rect locked (at -5.755 0.589498 90) (size 1.17 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "G3" smd rect locked (at -3.73 11.074999 90) (size 1.9 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "G4" smd rect locked (at 2.240001 11.074999 90) (size 1.9 1.35) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "G5" smd rect locked (at 5.740002 10.1 90) (size 1.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 131 "GND"))
    (pad "G6" smd rect locked (at 5.740002 6.4 90) (size 1.2 1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 108 "SDC0_DET"))
  )
  (footprint "LIB_MANGO.IntLib:C0402" (layer "B.Cu")
    (tedit 0)
    (at 76.326399 136.962003)
    (fp_text reference "C12" (at -1.7907 3.5687 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 3.3147 6.3627 90 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "NetC12_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/0402 SMD Capacitor.step"
      (offset (xyz 0.017399 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 57.276399 142.169003 180)
    (fp_text reference "R45" (at 0.8763 1.536705 unlocked) (layer "B.SilkS") hide)
    (fp_text value "NC" (at 0.8763 -3.035295 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.457197 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "NetR23_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 180) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "NetC4_2") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 60.6282 146.385403 90)
    (fp_text reference "R11" (at 1.536702 0.114298 unlocked) (layer "B.SilkS") hide)
    (fp_text value "150K 1%" (at -3.3147 0.1143 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000003 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "NetR10_2") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000003 90) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 131 "GND") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (footprint "LIB_MANGO.IntLib:R0402" (layer "B.Cu")
    (tedit 0)
    (at 75.920001 117.073803 -90)
    (fp_text reference "R82" (at -1.5367 -0.0381 unlocked) (layer "B.SilkS") hide)
    (fp_text value "10K" (at 3.0353 -0.0381 unlocked) (layer "B.SilkS") hide)
    (pad "1" smd roundrect (at -0.4572 0.000002 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 57 "CTP_INT") (solder_mask_margin 0.0508))
    (pad "2" smd roundrect (at 0.4572 0.000002 270) (size 0.508 0.508) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 126 "VCC3V3") (solder_mask_margin 0.0508))
    (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/R0402.STEP"
      (offset (xyz 0.0254 -0.004001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 -0 0))
    )
  )
  (gr_line (start 88.002598 116.707205) (end 85.502598 116.707205) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 56.502598 116.707205) (end 54.002598 116.707204) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 91.002598 151.707204) (mid 90.123918 153.828524) (end 88.002598 154.707204) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 84.502598 115.707205) (end 84.502598 115.407203) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 57.502598 155.707203) (end 57.502598 156.007203) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 85.502598 154.707203) (end 88.002598 154.707204) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start -163.532004 268.528809) (end -163.532004 268.528809) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 84.502598 156.007203) (end 84.502598 155.707203) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 91.002595 119.707204) (end 91.002593 119.707204) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 88.002596 116.707208) (end 88.002598 116.707205) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start -163.532004 268.528809) (end -163.532004 268.528809) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 91.002597 151.707204) (end 91.002595 119.707204) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 54.002598 154.707204) (mid 51.881278 153.828524) (end 51.002598 151.707204) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 84.502598 115.407203) (end 57.502598 115.407203) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 88.002597 116.707207) (mid 90.123915 117.585886) (end 91.002593 119.707204) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 56.502598 154.707203) (end 57.502598 155.707203) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 57.502598 115.407203) (end 57.502598 115.707205) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 57.502598 156.007203) (end 84.502598 156.007203) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 85.502598 116.707205) (end 84.502598 115.707205) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 54.002598 154.707203) (end 56.502598 154.707203) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 51.002599 151.707204) (end 51.002598 151.707204) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start -163.532004 268.528809) (end -163.532004 268.528809) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 51.002599 119.707204) (end 51.002599 151.707204) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 84.502598 155.707203) (end 85.502598 154.707203) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 57.502598 115.707205) (end 56.502598 116.707205) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start -163.532004 268.528809) (end -163.532004 268.528809) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 51.002598 119.707204) (mid 51.881278 117.585884) (end 54.002598 116.707204) (layer "Edge.Cuts") (width 0.05))
  (gr_text "G" (at 76.243996 126.852803) (layer "B.SilkS"))
  (gr_text "3" (at 88.435996 147.426803) (layer "B.SilkS"))
  (gr_text "mangopi.org" (at 81.831996 149.148809) (layer "B.SilkS"))
  (gr_text "RO" (at 80.314199 123.804803) (layer "B.SilkS"))
  (gr_text "SPK" (at 88.721599 123.068203) (layer "B.SilkS"))
  (gr_text "R" (at 88.696199 148.773003) (layer "B.SilkS"))
  (gr_text "RST" (at 53.764996 144.703809 270) (layer "B.SilkS"))
  (gr_text "CTP" (at 84.124199 122.509403) (layer "B.SilkS"))
  (gr_text "1" (at 70.712999 140.721198 270) (layer "B.SilkS"))
  (gr_text "+" (at 65.226599 137.004282) (layer "B.SilkS"))
  (gr_text "TVIN" (at 75.361199 126.852803) (layer "B.SilkS"))
  (gr_text "TF" (at 52.113996 136.067809 270) (layer "B.SilkS"))
  (gr_text "LO" (at 79.806199 126.954403) (layer "B.SilkS"))
  (gr_text "T" (at 87.927996 148.773003) (layer "B.SilkS"))
  (gr_text "FEL" (at 53.764996 126.669809 270) (layer "B.SilkS"))
  (gr_text "DVP" (at 72.897399 148.519003) (layer "B.SilkS"))
  (gr_text "Nezha-MQ" (at 82.085996 138.861809 45) (layer "F.SilkS"))
  (gr_text "7" (at 66.931757 123.101338) (layer "F.SilkS"))
  (gr_text "1" (at 59.257599 155.224603) (layer "F.SilkS"))
  (gr_text "14" (at 74.270584 117.045188) (layer "F.SilkS"))
  (gr_text "T" (at 66.801399 155.224603) (layer "F.SilkS"))
  (gr_text "L" (at 84.378199 134.676003) (layer "F.SilkS"))
  (gr_text "X" (at 73.252999 146.055203) (layer "F.SilkS"))
  (gr_text "SPK" (at 87.375399 123.144403) (layer "F.SilkS"))
  (gr_text "3" (at 87.807199 147.426803) (layer "F.SilkS"))
  (gr_text "14" (at 74.270584 148.898187) (layer "F.SilkS"))
  (gr_text "13" (at 73.957996 155.244809) (layer "F.SilkS"))
  (gr_text "TV" (at 79.374399 136.073003) (layer "F.SilkS"))
  (gr_text "P2" (at 72.059199 124.465203) (layer "F.SilkS"))
  (gr_text "20" (at 81.837752 148.898187) (layer "F.SilkS"))
  (gr_text "13:21" (at 70.655996 132.384809) (layer "F.SilkS"))
  (gr_text "R" (at 88.365999 148.773003) (layer "F.SilkS"))
  (gr_text "2" (at 59.114424 148.898187) (layer "F.SilkS"))
  (gr_text "G" (at 82.955799 136.047603) (layer "F.SilkS"))
  (gr_text "1" (at 59.257599 123.109262) (layer "F.SilkS"))
  (gr_text "G" (at 79.882399 134.650603) (layer "F.SilkS"))
  (gr_text "P3" (at 72.059199 147.858603) (layer "F.SilkS"))
  (gr_text "PWM7" (at 52.602799 137.444603) (layer "F.SilkS"))
  (gr_text "PWR" (at 52.602799 134.472803) (layer "F.SilkS"))
  (gr_text "OTG" (at 53.034599 123.398403) (layer "F.SilkS"))
  (gr_text "20" (at 81.837752 117.053112) (layer "F.SilkS"))
  (gr_text "8" (at 66.925945 117.053112) (layer "F.SilkS"))
  (gr_text "19" (at 81.888999 155.224603) (layer "F.SilkS"))
  (gr_text "2" (at 59.114424 117.045188) (layer "F.SilkS"))
  (gr_text "19" (at 81.888999 123.168516) (layer "F.SilkS"))
  (gr_text "T" (at 87.476999 148.773003) (layer "F.SilkS"))
  (gr_text "ANT" (at 59.638599 129.697603) (layer "F.SilkS"))
  (gr_text "HOST" (at 52.628199 148.823803) (layer "F.SilkS"))
  (gr_text "13" (at 74.268999 123.117716) (layer "F.SilkS"))
  (gr_text "R" (at 66.801399 148.898187) (layer "F.SilkS"))
  (gr_text "R" (at 82.803399 135.260203) (layer "F.SilkS"))
  (gr_text "MangoPi" (at 68.623996 145.846809) (layer "F.SilkS"))
  (gr_text "V1.6-211219" (at 82.720996 139.623809 45) (layer "F.SilkS"))
  (dimension (type aligned) (layer "F.SilkS")
    (pts (xy 84.502598 115.707205) (xy 84.502598 155.707203))
    (height -11.813601)
    (gr_text "40.0000 mm" (at 94.166199 135.707204 90) (layer "F.SilkS"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.05) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "F.SilkS")
    (pts (xy 51.002599 119.707204) (xy 91.002593 119.707204))
    (height -9.547001)
    (gr_text "40.0000 mm" (at 71.002596 108.010203) (layer "F.SilkS"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.05) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 131) (net_name "GND") (layer "In1.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 84.078166 115.990801)
        (xy 84.141648 116.068154)
        (xy 85.141649 117.068154)
        (xy 85.219002 117.131637)
        (xy 85.307254 117.178807)
        (xy 85.403012 117.207857)
        (xy 85.502598 117.217664)
        (xy 88.00257 117.217664)
        (xy 88.002596 117.217666)
        (xy 88.018715 117.216079)
        (xy 88.219773 117.224857)
        (xy 88.435298 117.253231)
        (xy 88.64753 117.300282)
        (xy 88.854852 117.365652)
        (xy 89.055687 117.448839)
        (xy 89.248512 117.549218)
        (xy 89.431851 117.666017)
        (xy 89.604312 117.798354)
        (xy 89.764586 117.945214)
        (xy 89.911446 118.105488)
        (xy 90.043783 118.277949)
        (xy 90.160582 118.461291)
        (xy 90.260961 118.654113)
        (xy 90.344148 118.854948)
        (xy 90.409518 119.06227)
        (xy 90.456569 119.274502)
        (xy 90.484943 119.490027)
        (xy 90.493721 119.691088)
        (xy 90.492134 119.707204)
        (xy 90.492136 119.70723)
        (xy 90.492139 151.707204)
        (xy 90.493726 151.72332)
        (xy 90.484948 151.924381)
        (xy 90.456574 152.139905)
        (xy 90.409523 152.352138)
        (xy 90.344153 152.55946)
        (xy 90.260966 152.760298)
        (xy 90.160587 152.953119)
        (xy 90.043788 153.136459)
        (xy 89.911452 153.308923)
        (xy 89.764589 153.469194)
        (xy 89.604317 153.616057)
        (xy 89.431854 153.748393)
        (xy 89.248514 153.865193)
        (xy 89.055692 153.965571)
        (xy 88.854855 154.048759)
        (xy 88.647532 154.114128)
        (xy 88.4353 154.161179)
        (xy 88.219776 154.189553)
        (xy 88.018715 154.198332)
        (xy 88.002598 154.196744)
        (xy 85.502598 154.196744)
        (xy 85.403012 154.206551)
        (xy 85.307254 154.235601)
        (xy 85.219002 154.282771)
        (xy 85.141649 154.346254)
        (xy 84.141648 155.346254)
        (xy 84.078166 155.423607)
        (xy 84.039076 155.496744)
        (xy 57.96612 155.496744)
        (xy 57.92703 155.423607)
        (xy 57.863548 155.346254)
        (xy 56.863547 154.346254)
        (xy 56.786194 154.282771)
        (xy 56.697942 154.235601)
        (xy 56.602184 154.206551)
        (xy 56.502598 154.196744)
        (xy 54.002598 154.196744)
        (xy 53.986481 154.198332)
        (xy 53.78542 154.189553)
        (xy 53.569896 154.161179)
        (xy 53.357664 154.114128)
        (xy 53.150341 154.048759)
        (xy 52.949504 153.965571)
        (xy 52.756682 153.865193)
        (xy 52.573342 153.748393)
        (xy 52.400879 153.616057)
        (xy 52.240607 153.469194)
        (xy 52.093745 153.308923)
        (xy 51.961408 153.136459)
        (xy 51.844609 152.953119)
        (xy 51.74423 152.760298)
        (xy 51.661043 152.55946)
        (xy 51.595673 152.352138)
        (xy 51.548622 152.139905)
        (xy 51.520248 151.924381)
        (xy 51.51147 151.72332)
        (xy 51.513057 151.707204)
        (xy 51.513057 119.707204)
        (xy 51.51147 119.691088)
        (xy 51.520248 119.490027)
        (xy 51.548622 119.274502)
        (xy 51.595673 119.06227)
        (xy 51.661043 118.854948)
        (xy 51.74423 118.65411)
        (xy 51.844609 118.461288)
        (xy 51.961408 118.277949)
        (xy 52.093745 118.105485)
        (xy 52.240607 117.945214)
        (xy 52.400879 117.798351)
        (xy 52.573342 117.666014)
        (xy 52.756682 117.549215)
        (xy 52.949504 117.448837)
        (xy 53.150341 117.365649)
        (xy 53.357664 117.30028)
        (xy 53.569896 117.253229)
        (xy 53.78542 117.224855)
        (xy 53.986481 117.216076)
        (xy 54.002598 117.217664)
        (xy 56.502598 117.217664)
        (xy 56.602184 117.207857)
        (xy 56.697942 117.178807)
        (xy 56.786194 117.131637)
        (xy 56.863547 117.068154)
        (xy 57.863548 116.068154)
        (xy 57.92703 115.990801)
        (xy 57.966123 115.917661)
        (xy 84.039073 115.917661)
      )
    )
  )
  (zone (net 131) (net_name "GND") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 90.575799 122.280405)
        (xy 90.575799 149.154003)
        (xy 90.555799 149.154003)
        (xy 84.485199 155.224603)
        (xy 57.519996 155.224603)
        (xy 51.510599 149.215205)
        (xy 51.510599 122.199203)
        (xy 57.728199 115.981603)
        (xy 84.276996 115.981603)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Paste") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.802604 137.0072)
        (xy 69.652589 137.0072)
        (xy 69.652589 136.8072)
        (xy 68.802604 136.8072)
        (xy 68.802604 135.807202)
        (xy 69.652589 135.807202)
        (xy 69.652589 135.607203)
        (xy 68.852591 135.607203)
        (xy 68.802604 135.607203)
        (xy 68.802604 134.607205)
        (xy 68.852591 134.607205)
        (xy 69.652589 134.607205)
        (xy 69.652589 134.407205)
        (xy 68.802604 134.407205)
        (xy 68.802604 133.507207)
        (xy 69.702602 133.507207)
        (xy 69.702602 134.357193)
        (xy 69.902602 134.357193)
        (xy 69.902602 133.507207)
        (xy 70.9026 133.507207)
        (xy 70.9026 134.357193)
        (xy 71.102599 134.357193)
        (xy 71.102599 133.507207)
        (xy 72.102597 133.507207)
        (xy 72.102597 134.357193)
        (xy 72.302597 134.357193)
        (xy 72.302597 133.507207)
        (xy 73.202595 133.507207)
        (xy 73.202595 134.407205)
        (xy 69.702602 134.407205)
        (xy 69.702602 135.55719)
        (xy 69.902602 135.55719)
        (xy 69.902602 134.607205)
        (xy 70.9026 134.607205)
        (xy 70.9026 135.55719)
        (xy 71.102599 135.55719)
        (xy 71.102599 134.607205)
        (xy 72.102597 134.607205)
        (xy 72.102597 135.55719)
        (xy 72.302597 135.55719)
        (xy 72.302597 134.607205)
        (xy 73.202595 134.607205)
        (xy 73.202595 135.607203)
        (xy 69.702602 135.607203)
        (xy 69.702602 136.757213)
        (xy 69.902602 136.757213)
        (xy 69.902602 135.807202)
        (xy 70.9026 135.807202)
        (xy 70.9026 136.757213)
        (xy 71.102599 136.757213)
        (xy 71.102599 135.807202)
        (xy 72.102597 135.807202)
        (xy 72.102597 136.757213)
        (xy 72.302597 136.757213)
        (xy 72.302597 135.807202)
        (xy 73.202595 135.807202)
        (xy 73.202595 136.8072)
        (xy 69.702602 136.8072)
        (xy 69.702602 137.857211)
        (xy 69.902602 137.857211)
        (xy 69.902602 137.0072)
        (xy 70.9026 137.0072)
        (xy 70.9026 137.857211)
        (xy 71.102599 137.857211)
        (xy 71.102599 137.0072)
        (xy 72.102597 137.0072)
        (xy 72.102597 137.807198)
        (xy 72.102597 137.857211)
        (xy 72.302597 137.857211)
        (xy 72.302597 137.807198)
        (xy 72.302597 137.0072)
        (xy 73.202595 137.0072)
        (xy 73.202595 137.907198)
        (xy 71.402599 137.907198)
        (xy 68.802604 137.907198)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55.390796 130.868847)
        (xy 55.476744 130.782899)
        (xy 55.585046 130.727717)
        (xy 55.705099 130.708702)
        (xy 55.825152 130.727717)
        (xy 55.933454 130.782899)
        (xy 56.019402 130.868847)
        (xy 56.074584 130.977149)
        (xy 56.093599 131.097202)
        (xy 56.074584 131.217255)
        (xy 56.019402 131.325557)
        (xy 55.933454 131.411505)
        (xy 55.825152 131.466687)
        (xy 55.705099 131.485702)
        (xy 55.585046 131.466687)
        (xy 55.476744 131.411505)
        (xy 55.390796 131.325557)
        (xy 55.335614 131.217255)
        (xy 55.316599 131.097202)
        (xy 55.335614 130.977149)
      )
    )
    (polygon
      (pts
        (xy 55.516568 131.285733)
        (xy 55.603067 131.34353)
        (xy 55.705099 131.363825)
        (xy 55.807131 131.34353)
        (xy 55.89363 131.285733)
        (xy 55.951427 131.199234)
        (xy 55.971722 131.097202)
        (xy 55.951427 130.99517)
        (xy 55.89363 130.908671)
        (xy 55.807131 130.850874)
        (xy 55.705099 130.830579)
        (xy 55.603067 130.850874)
        (xy 55.516568 130.908671)
        (xy 55.458771 130.99517)
        (xy 55.438476 131.097202)
        (xy 55.458771 131.199234)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51.047499 151.662303)
        (xy 51.066098 151.707204)
        (xy 51.062023 151.717041)
        (xy 51.079964 152.036506)
        (xy 51.135211 152.361666)
        (xy 51.226517 152.678597)
        (xy 51.352734 152.983311)
        (xy 51.512275 153.271978)
        (xy 51.703133 153.540966)
        (xy 51.922907 153.786895)
        (xy 52.168836 154.006669)
        (xy 52.437824 154.197527)
        (xy 52.726491 154.357068)
        (xy 53.031205 154.483285)
        (xy 53.348136 154.574591)
        (xy 53.673296 154.629838)
        (xy 53.992761 154.647779)
        (xy 54.002598 154.643704)
        (xy 54.047499 154.662303)
        (xy 54.066098 154.707204)
        (xy 54.047499 154.752105)
        (xy 54.002598 154.770704)
        (xy 53.682375 154.753922)
        (xy 53.365661 154.703759)
        (xy 53.055925 154.620765)
        (xy 52.75656 154.50585)
        (xy 52.470848 154.360273)
        (xy 52.201918 154.185627)
        (xy 51.952717 153.983828)
        (xy 51.725974 153.757085)
        (xy 51.524175 153.507884)
        (xy 51.349529 153.238954)
        (xy 51.203952 152.953242)
        (xy 51.089037 152.653877)
        (xy 51.006043 152.344141)
        (xy 50.95588 152.027427)
        (xy 50.939098 151.707204)
        (xy 50.957697 151.662303)
        (xy 51.002598 151.643704)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55.390796 125.088848)
        (xy 55.476744 125.0029)
        (xy 55.585046 124.947718)
        (xy 55.705099 124.928703)
        (xy 55.825152 124.947718)
        (xy 55.933454 125.0029)
        (xy 56.019402 125.088848)
        (xy 56.074584 125.19715)
        (xy 56.093599 125.317203)
        (xy 56.074584 125.437256)
        (xy 56.019402 125.545558)
        (xy 55.933454 125.631506)
        (xy 55.825152 125.686688)
        (xy 55.705099 125.705703)
        (xy 55.585046 125.686688)
        (xy 55.476744 125.631506)
        (xy 55.390796 125.545558)
        (xy 55.335614 125.437256)
        (xy 55.316599 125.317203)
        (xy 55.335614 125.19715)
      )
    )
    (polygon
      (pts
        (xy 55.516568 125.505734)
        (xy 55.603067 125.563531)
        (xy 55.705099 125.583826)
        (xy 55.807131 125.563531)
        (xy 55.89363 125.505734)
        (xy 55.951427 125.419235)
        (xy 55.971722 125.317203)
        (xy 55.951427 125.215171)
        (xy 55.89363 125.128672)
        (xy 55.807131 125.070875)
        (xy 55.705099 125.05058)
        (xy 55.603067 125.070875)
        (xy 55.516568 125.128672)
        (xy 55.458771 125.215171)
        (xy 55.438476 125.317203)
        (xy 55.458771 125.419235)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.047499 154.662302)
        (xy 88.066098 154.707203)
        (xy 88.047499 154.752104)
        (xy 88.002598 154.770703)
        (xy 85.502598 154.770703)
        (xy 85.457697 154.752104)
        (xy 85.439098 154.707203)
        (xy 85.457697 154.662302)
        (xy 85.502598 154.643703)
        (xy 88.002598 154.643703)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51.678992 125.622088)
        (xy 51.767485 125.533595)
        (xy 51.878992 125.476779)
        (xy 52.002599 125.457202)
        (xy 52.126206 125.476779)
        (xy 52.237713 125.533595)
        (xy 52.326206 125.622088)
        (xy 52.383022 125.733595)
        (xy 52.402599 125.857202)
        (xy 52.383022 125.980809)
        (xy 52.326206 126.092316)
        (xy 52.237713 126.180809)
        (xy 52.126206 126.237625)
        (xy 52.002599 126.257202)
        (xy 51.878992 126.237625)
        (xy 51.767485 126.180809)
        (xy 51.678992 126.092316)
        (xy 51.622176 125.980809)
        (xy 51.602599 125.857202)
        (xy 51.622176 125.733595)
      )
    )
    (polygon
      (pts
        (xy 51.76924 126.053013)
        (xy 51.850285 126.121018)
        (xy 51.949701 126.157202)
        (xy 52.055497 126.157202)
        (xy 52.154913 126.121018)
        (xy 52.235958 126.053013)
        (xy 52.288856 125.961391)
        (xy 52.307227 125.857202)
        (xy 52.288856 125.753013)
        (xy 52.235958 125.661391)
        (xy 52.154913 125.593386)
        (xy 52.055497 125.557202)
        (xy 51.949701 125.557202)
        (xy 51.850285 125.593386)
        (xy 51.76924 125.661391)
        (xy 51.716342 125.753013)
        (xy 51.697971 125.857202)
        (xy 51.716342 125.961391)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57.502598 115.643705)
        (xy 57.5475 115.662303)
        (xy 57.566098 115.707205)
        (xy 57.5475 115.752106)
        (xy 56.547499 116.752106)
        (xy 56.502598 116.770705)
        (xy 56.457697 116.752106)
        (xy 56.439098 116.707205)
        (xy 56.457697 116.662304)
        (xy 57.457697 115.662303)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56.547499 116.662304)
        (xy 56.566098 116.707205)
        (xy 56.547499 116.752106)
        (xy 56.502598 116.770705)
        (xy 54.002598 116.770705)
        (xy 53.957697 116.752106)
        (xy 53.939098 116.707205)
        (xy 53.957697 116.662304)
        (xy 54.002598 116.643705)
        (xy 56.502598 116.643705)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.047498 151.752105)
        (xy 91.002597 151.770704)
        (xy 90.957696 151.752105)
        (xy 90.939097 151.707204)
        (xy 90.939095 119.707204)
        (xy 90.957694 119.662303)
        (xy 91.002595 119.643704)
        (xy 91.047496 119.662303)
        (xy 91.066095 119.707204)
        (xy 91.066097 151.707204)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.047499 116.662304)
        (xy 88.066098 116.707205)
        (xy 88.047499 116.752106)
        (xy 88.002598 116.770705)
        (xy 85.502598 116.770705)
        (xy 85.457697 116.752106)
        (xy 85.439098 116.707205)
        (xy 85.457697 116.662304)
        (xy 85.502598 116.643705)
        (xy 88.002598 116.643705)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55.390796 145.868847)
        (xy 55.476744 145.782899)
        (xy 55.585046 145.727717)
        (xy 55.705099 145.708702)
        (xy 55.825152 145.727717)
        (xy 55.933454 145.782899)
        (xy 56.019402 145.868847)
        (xy 56.074584 145.977149)
        (xy 56.093599 146.097202)
        (xy 56.074584 146.217255)
        (xy 56.019402 146.325557)
        (xy 55.933454 146.411505)
        (xy 55.825152 146.466687)
        (xy 55.705099 146.485702)
        (xy 55.585046 146.466687)
        (xy 55.476744 146.411505)
        (xy 55.390796 146.325557)
        (xy 55.335614 146.217255)
        (xy 55.316599 146.097202)
        (xy 55.335614 145.977149)
      )
    )
    (polygon
      (pts
        (xy 55.516568 146.285733)
        (xy 55.603067 146.34353)
        (xy 55.705099 146.363825)
        (xy 55.807131 146.34353)
        (xy 55.89363 146.285733)
        (xy 55.951427 146.199234)
        (xy 55.971722 146.097202)
        (xy 55.951427 145.99517)
        (xy 55.89363 145.908671)
        (xy 55.807131 145.850874)
        (xy 55.705099 145.830579)
        (xy 55.603067 145.850874)
        (xy 55.516568 145.908671)
        (xy 55.458771 145.99517)
        (xy 55.438476 146.097202)
        (xy 55.458771 146.199234)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57.566098 155.707203)
        (xy 57.5475 155.752105)
        (xy 57.502598 155.770703)
        (xy 57.457697 155.752105)
        (xy 56.457697 154.752104)
        (xy 56.439098 154.707203)
        (xy 56.457697 154.662302)
        (xy 56.502598 154.643703)
        (xy 56.547499 154.662302)
        (xy 57.5475 155.662302)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.957698 133.562303)
        (xy 51.002599 133.543704)
        (xy 51.0475 133.562303)
        (xy 51.066099 133.607204)
        (xy 51.066099 151.707204)
        (xy 51.0475 151.752105)
        (xy 51.002599 151.770704)
        (xy 50.957698 151.752105)
        (xy 50.939099 151.707204)
        (xy 50.939099 133.607204)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55.390796 140.088849)
        (xy 55.476744 140.002901)
        (xy 55.585046 139.947719)
        (xy 55.705099 139.928704)
        (xy 55.825152 139.947719)
        (xy 55.933454 140.002901)
        (xy 56.019402 140.088849)
        (xy 56.074584 140.197151)
        (xy 56.093599 140.317204)
        (xy 56.074584 140.437257)
        (xy 56.019402 140.545559)
        (xy 55.933454 140.631507)
        (xy 55.825152 140.686689)
        (xy 55.705099 140.705704)
        (xy 55.585046 140.686689)
        (xy 55.476744 140.631507)
        (xy 55.390796 140.545559)
        (xy 55.335614 140.437257)
        (xy 55.316599 140.317204)
        (xy 55.335614 140.197151)
      )
    )
    (polygon
      (pts
        (xy 55.516568 140.505735)
        (xy 55.603067 140.563532)
        (xy 55.705099 140.583827)
        (xy 55.807131 140.563532)
        (xy 55.89363 140.505735)
        (xy 55.951427 140.419236)
        (xy 55.971722 140.317204)
        (xy 55.951427 140.215172)
        (xy 55.89363 140.128673)
        (xy 55.807131 140.070876)
        (xy 55.705099 140.050581)
        (xy 55.603067 140.070876)
        (xy 55.516568 140.128673)
        (xy 55.458771 140.215172)
        (xy 55.438476 140.317204)
        (xy 55.458771 140.419236)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.547499 115.662304)
        (xy 84.566098 115.707205)
        (xy 84.547499 115.752106)
        (xy 84.502598 115.770705)
        (xy 57.502598 115.770705)
        (xy 57.457697 115.752106)
        (xy 57.439098 115.707205)
        (xy 57.457697 115.662304)
        (xy 57.502598 115.643705)
        (xy 84.502598 115.643705)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51.678992 145.322089)
        (xy 51.767485 145.233596)
        (xy 51.878992 145.17678)
        (xy 52.002599 145.157203)
        (xy 52.126206 145.17678)
        (xy 52.237713 145.233596)
        (xy 52.326206 145.322089)
        (xy 52.383022 145.433596)
        (xy 52.402599 145.557203)
        (xy 52.383022 145.68081)
        (xy 52.326206 145.792317)
        (xy 52.237713 145.88081)
        (xy 52.126206 145.937626)
        (xy 52.002599 145.957203)
        (xy 51.878992 145.937626)
        (xy 51.767485 145.88081)
        (xy 51.678992 145.792317)
        (xy 51.622176 145.68081)
        (xy 51.602599 145.557203)
        (xy 51.622176 145.433596)
      )
    )
    (polygon
      (pts
        (xy 51.76924 145.753014)
        (xy 51.850285 145.821019)
        (xy 51.949701 145.857203)
        (xy 52.055497 145.857203)
        (xy 52.154913 145.821019)
        (xy 52.235958 145.753014)
        (xy 52.288856 145.661392)
        (xy 52.307227 145.557203)
        (xy 52.288856 145.453014)
        (xy 52.235958 145.361392)
        (xy 52.154913 145.293387)
        (xy 52.055497 145.257203)
        (xy 51.949701 145.257203)
        (xy 51.850285 145.293387)
        (xy 51.76924 145.361392)
        (xy 51.716342 145.453014)
        (xy 51.697971 145.557203)
        (xy 51.716342 145.661392)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.957698 119.662303)
        (xy 51.002599 119.643704)
        (xy 51.0475 119.662303)
        (xy 51.066099 119.707204)
        (xy 51.066099 127.207204)
        (xy 51.0475 127.252105)
        (xy 51.002599 127.270704)
        (xy 50.957698 127.252105)
        (xy 50.939099 127.207204)
        (xy 50.939099 119.707204)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.502598 154.643703)
        (xy 85.5475 154.662301)
        (xy 85.566098 154.707203)
        (xy 85.5475 154.752104)
        (xy 84.547499 155.752104)
        (xy 84.502598 155.770703)
        (xy 84.457697 155.752104)
        (xy 84.439098 155.707203)
        (xy 84.457697 155.662302)
        (xy 85.457697 154.662301)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.547499 155.662302)
        (xy 84.566098 155.707203)
        (xy 84.547499 155.752104)
        (xy 84.502598 155.770703)
        (xy 57.502598 155.770703)
        (xy 57.457697 155.752104)
        (xy 57.439098 155.707203)
        (xy 57.457697 155.662302)
        (xy 57.502598 155.643703)
        (xy 84.502598 155.643703)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.566098 116.707205)
        (xy 85.5475 116.752107)
        (xy 85.502598 116.770705)
        (xy 85.457697 116.752107)
        (xy 84.457697 115.752106)
        (xy 84.439098 115.707205)
        (xy 84.457697 115.662304)
        (xy 84.502598 115.643705)
        (xy 84.547499 115.662304)
        (xy 85.5475 116.662304)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.322821 116.660486)
        (xy 88.639535 116.710649)
        (xy 88.949271 116.793643)
        (xy 89.248636 116.908558)
        (xy 89.534348 117.054135)
        (xy 89.803278 117.228781)
        (xy 90.052479 117.43058)
        (xy 90.279222 117.657323)
        (xy 90.481021 117.906524)
        (xy 90.655667 118.175454)
        (xy 90.801244 118.461166)
        (xy 90.916159 118.760531)
        (xy 90.999153 119.070267)
        (xy 91.049316 119.386981)
        (xy 91.066098 119.707204)
        (xy 91.047499 119.752105)
        (xy 91.002598 119.770704)
        (xy 90.957697 119.752105)
        (xy 90.939098 119.707204)
        (xy 90.943173 119.697367)
        (xy 90.925232 119.377902)
        (xy 90.869985 119.052742)
        (xy 90.778679 118.735811)
        (xy 90.652462 118.431097)
        (xy 90.492921 118.14243)
        (xy 90.302063 117.873442)
        (xy 90.082289 117.627513)
        (xy 89.83636 117.407739)
        (xy 89.567372 117.216881)
        (xy 89.278705 117.05734)
        (xy 88.973991 116.931123)
        (xy 88.65706 116.839817)
        (xy 88.3319 116.78457)
        (xy 88.012435 116.766629)
        (xy 88.002598 116.770704)
        (xy 87.957697 116.752105)
        (xy 87.939098 116.707204)
        (xy 87.957697 116.662303)
        (xy 88.002598 116.643704)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51.678992 143.622088)
        (xy 51.767485 143.533595)
        (xy 51.878992 143.476779)
        (xy 52.002599 143.457202)
        (xy 52.126206 143.476779)
        (xy 52.237713 143.533595)
        (xy 52.326206 143.622088)
        (xy 52.383022 143.733595)
        (xy 52.402599 143.857202)
        (xy 52.383022 143.980809)
        (xy 52.326206 144.092316)
        (xy 52.237713 144.180809)
        (xy 52.126206 144.237625)
        (xy 52.002599 144.257202)
        (xy 51.878992 144.237625)
        (xy 51.767485 144.180809)
        (xy 51.678992 144.092316)
        (xy 51.622176 143.980809)
        (xy 51.602599 143.857202)
        (xy 51.622176 143.733595)
      )
    )
    (polygon
      (pts
        (xy 51.76924 144.053013)
        (xy 51.850285 144.121018)
        (xy 51.949701 144.157202)
        (xy 52.055497 144.157202)
        (xy 52.154913 144.121018)
        (xy 52.235958 144.053013)
        (xy 52.288856 143.961391)
        (xy 52.307227 143.857202)
        (xy 52.288856 143.753013)
        (xy 52.235958 143.661391)
        (xy 52.154913 143.593386)
        (xy 52.055497 143.557202)
        (xy 51.949701 143.557202)
        (xy 51.850285 143.593386)
        (xy 51.76924 143.661391)
        (xy 51.716342 143.753013)
        (xy 51.697971 143.857202)
        (xy 51.716342 143.961391)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56.547499 154.662302)
        (xy 56.566098 154.707203)
        (xy 56.547499 154.752104)
        (xy 56.502598 154.770703)
        (xy 54.002598 154.770703)
        (xy 53.957697 154.752104)
        (xy 53.939098 154.707203)
        (xy 53.957697 154.662302)
        (xy 54.002598 154.643703)
        (xy 56.502598 154.643703)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.047499 116.662303)
        (xy 54.066098 116.707204)
        (xy 54.047499 116.752105)
        (xy 54.002598 116.770704)
        (xy 53.992761 116.766629)
        (xy 53.673296 116.78457)
        (xy 53.348136 116.839817)
        (xy 53.031205 116.931123)
        (xy 52.726491 117.05734)
        (xy 52.437824 117.216881)
        (xy 52.168836 117.407739)
        (xy 51.922907 117.627513)
        (xy 51.703133 117.873442)
        (xy 51.512275 118.14243)
        (xy 51.352734 118.431097)
        (xy 51.226517 118.735811)
        (xy 51.135211 119.052742)
        (xy 51.079964 119.377902)
        (xy 51.062023 119.697367)
        (xy 51.066098 119.707204)
        (xy 51.047499 119.752105)
        (xy 51.002598 119.770704)
        (xy 50.957697 119.752105)
        (xy 50.939098 119.707204)
        (xy 50.95588 119.386981)
        (xy 51.006043 119.070267)
        (xy 51.089037 118.760531)
        (xy 51.203952 118.461166)
        (xy 51.349529 118.175454)
        (xy 51.524175 117.906524)
        (xy 51.725974 117.657323)
        (xy 51.952717 117.43058)
        (xy 52.201918 117.228781)
        (xy 52.470848 117.054135)
        (xy 52.75656 116.908558)
        (xy 53.055925 116.793643)
        (xy 53.365661 116.710649)
        (xy 53.682375 116.660486)
        (xy 54.002598 116.643704)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.047499 151.662303)
        (xy 91.066098 151.707204)
        (xy 91.049316 152.027427)
        (xy 90.999153 152.344141)
        (xy 90.916159 152.653877)
        (xy 90.801244 152.953242)
        (xy 90.655667 153.238954)
        (xy 90.481021 153.507884)
        (xy 90.279222 153.757085)
        (xy 90.052479 153.983828)
        (xy 89.803278 154.185627)
        (xy 89.534348 154.360273)
        (xy 89.248636 154.50585)
        (xy 88.949271 154.620765)
        (xy 88.639535 154.703759)
        (xy 88.322821 154.753922)
        (xy 88.002598 154.770704)
        (xy 87.957697 154.752105)
        (xy 87.939098 154.707204)
        (xy 87.957697 154.662303)
        (xy 88.002598 154.643704)
        (xy 88.012435 154.647779)
        (xy 88.3319 154.629838)
        (xy 88.65706 154.574591)
        (xy 88.973991 154.483285)
        (xy 89.278705 154.357068)
        (xy 89.567372 154.197527)
        (xy 89.83636 154.006669)
        (xy 90.082289 153.786895)
        (xy 90.302063 153.540966)
        (xy 90.492921 153.271978)
        (xy 90.652462 152.983311)
        (xy 90.778679 152.678597)
        (xy 90.869985 152.361666)
        (xy 90.925232 152.036506)
        (xy 90.943173 151.717041)
        (xy 90.939098 151.707204)
        (xy 90.957697 151.662303)
        (xy 91.002598 151.643704)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61.375961 128.409821)
        (xy 61.375961 126.208911)
        (xy 60.977179 126.208913)
        (xy 60.977179 125.209423)
        (xy 60.424729 125.209423)
        (xy 59.876089 125.209423)
        (xy 59.876089 126.208913)
        (xy 59.476041 126.208913)
        (xy 59.476041 128.409823)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.957698 127.162303)
        (xy 51.002599 127.143704)
        (xy 51.0475 127.162303)
        (xy 51.066099 127.207204)
        (xy 51.066099 133.607204)
        (xy 51.0475 133.652105)
        (xy 51.002599 133.670704)
        (xy 50.957698 133.652105)
        (xy 50.939099 133.607204)
        (xy 50.939099 127.207204)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "Margin") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51.678992 127.32209)
        (xy 51.767485 127.233597)
        (xy 51.878992 127.176781)
        (xy 52.002599 127.157204)
        (xy 52.126206 127.176781)
        (xy 52.237713 127.233597)
        (xy 52.326206 127.32209)
        (xy 52.383022 127.433597)
        (xy 52.402599 127.557204)
        (xy 52.383022 127.680811)
        (xy 52.326206 127.792318)
        (xy 52.237713 127.880811)
        (xy 52.126206 127.937627)
        (xy 52.002599 127.957204)
        (xy 51.878992 127.937627)
        (xy 51.767485 127.880811)
        (xy 51.678992 127.792318)
        (xy 51.622176 127.680811)
        (xy 51.602599 127.557204)
        (xy 51.622176 127.433597)
      )
    )
    (polygon
      (pts
        (xy 51.76924 127.753015)
        (xy 51.850285 127.82102)
        (xy 51.949701 127.857204)
        (xy 52.055497 127.857204)
        (xy 52.154913 127.82102)
        (xy 52.235958 127.753015)
        (xy 52.288856 127.661393)
        (xy 52.307227 127.557204)
        (xy 52.288856 127.453015)
        (xy 52.235958 127.361393)
        (xy 52.154913 127.293388)
        (xy 52.055497 127.257204)
        (xy 51.949701 127.257204)
        (xy 51.850285 127.293388)
        (xy 51.76924 127.361393)
        (xy 51.716342 127.453015)
        (xy 51.697971 127.557204)
        (xy 51.716342 127.661393)
      )
    )
  )
)
