(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (title_block
    (title "RF")
    (date "20211125")
    (rev "V1.5")
  )
  (lib_symbols
    (symbol "WIFI-BT-altium-import:0_AP6212" (in_bom yes) (on_board yes)
      (property "Reference" "" (id 0) (at 0 0 0))
      (property "Value" "0_AP6212" (id 1) (at 0 0 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_fp_filters" "AP6212" (id 4) (at 0 0 0))
      (symbol "0_AP6212_1_0"
        (rectangle (start 55.88 55.88) (end 0 0)
          (fill (type background))
        )
        (pin passive line (at -5.08 40.64 0) (length 5.08)
          (name "GND")
          (number "1")
        )
        (pin passive line (at -5.08 17.78 0) (length 5.08)
          (name "XTAL_IN")
          (number "10")
        )
        (pin passive line (at -5.08 15.24 0) (length 5.08)
          (name "XTAL_OUT")
          (number "11")
        )
        (pin passive line (at 15.24 -5.08 90) (length 5.08)
          (name "WL_REG_ON")
          (number "12")
        )
        (pin passive line (at 17.78 -5.08 90) (length 5.08)
          (name "WL_HOST_WAKE")
          (number "13")
        )
        (pin passive line (at 20.32 -5.08 90) (length 5.08)
          (name "SDIO_DATA_2")
          (number "14")
        )
        (pin passive line (at 22.86 -5.08 90) (length 5.08)
          (name "SDIO_DATA_3")
          (number "15")
        )
        (pin passive line (at 25.4 -5.08 90) (length 5.08)
          (name "SDIO_DATA_CMD")
          (number "16")
        )
        (pin passive line (at 27.94 -5.08 90) (length 5.08)
          (name "SDIO_DATA_CLK")
          (number "17")
        )
        (pin passive line (at 30.48 -5.08 90) (length 5.08)
          (name "SDIO_DATA_0")
          (number "18")
        )
        (pin passive line (at 33.02 -5.08 90) (length 5.08)
          (name "SDIO_DATA_1")
          (number "19")
        )
        (pin passive line (at -5.08 38.1 0) (length 5.08)
          (name "WL_BT_ANT")
          (number "2")
        )
        (pin passive line (at 35.56 -5.08 90) (length 5.08)
          (name "GND")
          (number "20")
        )
        (pin passive line (at 38.1 -5.08 90) (length 5.08)
          (name "VIN_LDO_OUT")
          (number "21")
        )
        (pin passive line (at 40.64 -5.08 90) (length 5.08)
          (name "VDDIO")
          (number "22")
        )
        (pin passive line (at 60.96 15.24 180) (length 5.08)
          (name "VIN_LDO")
          (number "23")
        )
        (pin passive line (at 60.96 17.78 180) (length 5.08)
          (name "LPO")
          (number "24")
        )
        (pin passive line (at 60.96 20.32 180) (length 5.08)
          (name "PCM_OUT")
          (number "25")
        )
        (pin passive line (at 60.96 22.86 180) (length 5.08)
          (name "PCM_CLK")
          (number "26")
        )
        (pin passive line (at 60.96 25.4 180) (length 5.08)
          (name "PCM_IN")
          (number "27")
        )
        (pin passive line (at 60.96 27.94 180) (length 5.08)
          (name "PCM_SYNC")
          (number "28")
        )
        (pin passive line (at 60.96 30.48 180) (length 5.08)
          (name "VDD_TCXO")
          (number "29")
        )
        (pin passive line (at -5.08 35.56 0) (length 5.08)
          (name "GND")
          (number "3")
        )
        (pin passive line (at 60.96 33.02 180) (length 5.08)
          (name "TCXO_IN")
          (number "30")
        )
        (pin passive line (at 60.96 35.56 180) (length 5.08)
          (name "GND")
          (number "31")
        )
        (pin passive line (at 60.96 38.1 180) (length 5.08)
          (name "GPS_RF")
          (number "32")
        )
        (pin passive line (at 60.96 40.64 180) (length 5.08)
          (name "GND")
          (number "33")
        )
        (pin passive line (at 40.64 60.96 270) (length 5.08)
          (name "BT_RST_N")
          (number "34")
        )
        (pin passive line (at 38.1 60.96 270) (length 5.08)
          (name "N_I2C_SDA")
          (number "35")
        )
        (pin passive line (at 35.56 60.96 270) (length 5.08)
          (name "GND")
          (number "36")
        )
        (pin passive line (at 33.02 60.96 270) (length 5.08)
          (name "N_I2C_SCL")
          (number "37")
        )
        (pin passive line (at 30.48 60.96 270) (length 5.08)
          (name "N_REG_PU")
          (number "38")
        )
        (pin passive line (at 27.94 60.96 270) (length 5.08)
          (name "TX2")
          (number "39")
        )
        (pin passive line (at -5.08 33.02 0) (length 5.08)
          (name "FM_RX")
          (number "4")
        )
        (pin passive line (at 25.4 60.96 270) (length 5.08)
          (name "TX1")
          (number "40")
        )
        (pin passive line (at 22.86 60.96 270) (length 5.08)
          (name "UART_RTS_N")
          (number "41")
        )
        (pin passive line (at 20.32 60.96 270) (length 5.08)
          (name "UART_TXD")
          (number "42")
        )
        (pin passive line (at 17.78 60.96 270) (length 5.08)
          (name "UART_RXD")
          (number "43")
        )
        (pin passive line (at 15.24 60.96 270) (length 5.08)
          (name "UART_CTS_N")
          (number "44")
        )
        (pin passive line (at -5.08 30.48 0) (length 5.08)
          (name "N_WAKE")
          (number "5")
        )
        (pin passive line (at -5.08 27.94 0) (length 5.08)
          (name "BT_WAKE")
          (number "6")
        )
        (pin passive line (at -5.08 25.4 0) (length 5.08)
          (name "BT_HOST_WAKE")
          (number "7")
        )
        (pin passive line (at -5.08 22.86 0) (length 5.08)
          (name "BT_VIO/N_HOST_WAKE")
          (number "8")
        )
        (pin passive line (at -5.08 20.32 0) (length 5.08)
          (name "VBAT")
          (number "9")
        )
        (pin passive line (at 45.72 60.96 270) (length 5.08)
          (name "TP1")
          (number "TP1")
        )
        (pin passive line (at 48.26 60.96 270) (length 5.08)
          (name "TP2")
          (number "TP2")
        )
        (pin passive line (at 50.8 60.96 270) (length 5.08)
          (name "TP3")
          (number "TP3")
        )
      )
    )
    (symbol "WIFI-BT-altium-import:0_mirrored_MCX_IPEX" (in_bom yes) (on_board yes)
      (property "Reference" "" (id 0) (at 0 0 0))
      (property "Value" "0_mirrored_MCX_IPEX" (id 1) (at 0 0 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_fp_filters" "I-PEX{space}SOCKET" (id 4) (at 0 0 0))
      (symbol "0_mirrored_MCX_IPEX_1_0"
        (polyline
          (pts
            (xy 0 2.54)
            (xy -1.524 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 5.08)
            (xy -5.08 5.08)
            (xy -5.08 0)
            (xy 0 0)
          )
          (fill (type none))
        )
        (pin passive line (at 2.54 2.54 180) (length 2.54)
          (name "Signal")
          (number "1")
        )
        (pin power_in line (at -2.54 -5.08 90) (length 5.08)
          (name "GND")
          (number "2")
        )
        (pin power_in line (at -2.54 10.16 270) (length 5.08)
          (name "GND")
          (number "3")
        )
      )
    )
    (symbol "WIFI-BT-altium-import:0_mirrored_RES" (in_bom yes) (on_board yes)
      (property "Reference" "" (id 0) (at 0 0 0))
      (property "Value" "0_mirrored_RES" (id 1) (at 0 0 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_description" "普通电阻" (id 4) (at 0 0 0))
      (property "ki_fp_filters" "R0402" (id 5) (at 0 0 0))
      (symbol "0_mirrored_RES_1_0"
        (rectangle (start -2.794 1.016) (end -7.874 -1.016)
          (fill (type none))
        )
        (pin passive line (at -0.254 0 180) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin passive line (at -10.414 0 0) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "WIFI-BT-altium-import:1_RES" (in_bom yes) (on_board yes)
      (property "Reference" "" (id 0) (at 0 0 0))
      (property "Value" "1_RES" (id 1) (at 0 0 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_description" "普通电阻" (id 4) (at 0 0 0))
      (property "ki_fp_filters" "R0402" (id 5) (at 0 0 0))
      (symbol "1_RES_1_0"
        (rectangle (start 1.016 7.874) (end -1.016 2.794)
          (fill (type none))
        )
        (pin passive line (at 0 0.254 90) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin passive line (at 0 10.414 270) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "WIFI-BT-altium-import:2_CAP" (in_bom yes) (on_board yes)
      (property "Reference" "" (id 0) (at 0 0 0))
      (property "Value" "2_CAP" (id 1) (at 0 0 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_description" "普通小电容" (id 4) (at 0 0 0))
      (property "ki_fp_filters" "C0402" (id 5) (at 0 0 0))
      (symbol "2_CAP_1_0"
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -1.27)
            (xy 0 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0.762)
            (xy 0 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.032 -0.762)
            (xy -2.032 -0.762)
          )
          (fill (type none))
        )
        (pin passive line (at 0 -2.54 90) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 0 2.54 270) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "WIFI-BT-altium-import:2_RES" (in_bom yes) (on_board yes)
      (property "Reference" "" (id 0) (at 0 0 0))
      (property "Value" "2_RES" (id 1) (at 0 0 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_description" "普通电阻" (id 4) (at 0 0 0))
      (property "ki_fp_filters" "R0402" (id 5) (at 0 0 0))
      (symbol "2_RES_1_0"
        (rectangle (start -2.794 1.016) (end -7.874 -1.016)
          (fill (type none))
        )
        (pin passive line (at -0.254 0 180) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin passive line (at -10.414 0 0) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "WIFI-BT-altium-import:2_mirrored_RES" (in_bom yes) (on_board yes)
      (property "Reference" "" (id 0) (at 0 0 0))
      (property "Value" "2_mirrored_RES" (id 1) (at 0 0 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_description" "普通电阻" (id 4) (at 0 0 0))
      (property "ki_fp_filters" "R0402" (id 5) (at 0 0 0))
      (symbol "2_mirrored_RES_1_0"
        (rectangle (start 7.874 1.016) (end 2.794 -1.016)
          (fill (type none))
        )
        (pin passive line (at 0.254 0 0) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin passive line (at 10.414 0 180) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "WIFI-BT-altium-import:3_CAP" (in_bom yes) (on_board yes)
      (property "Reference" "" (id 0) (at 0 0 0))
      (property "Value" "3_CAP" (id 1) (at 0 0 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_description" "普通小电容" (id 4) (at 0 0 0))
      (property "ki_fp_filters" "C0402" (id 5) (at 0 0 0))
      (symbol "3_CAP_1_0"
        (polyline
          (pts
            (xy -0.762 -2.032)
            (xy -0.762 2.032)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.762 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 2.032)
            (xy 0.762 -2.032)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.762 0)
          )
          (fill (type none))
        )
        (pin passive line (at 2.54 0 180) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at -2.54 0 0) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "WIFI-BT-altium-import:GND" (power) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 0 0))
      (property "Value" "GND" (id 1) (at 0 6.35 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "电源符号创建名为 'GND' 的全局标签" (id 5) (at 0 0 0))
      (symbol "GND_0_0"
        (polyline
          (pts
            (xy -2.54 -2.54)
            (xy 2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -3.302)
            (xy 1.778 -3.302)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.016 -4.064)
            (xy 1.016 -4.064)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -0.254 -4.826)
            (xy 0.254 -4.826)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -2.54)
          )
          (fill (type none))
        )
        (pin power_in line (at 0 0 0) (length 0) hide
          (name "GND")
          (number "")
        )
      )
    )
    (symbol "WIFI-BT-altium-import:VCC3V3" (power) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 0 0))
      (property "Value" "VCC3V3" (id 1) (at 0 3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "电源符号创建名为 'VCC3V3' 的全局标签" (id 5) (at 0 0 0))
      (symbol "VCC3V3_0_0"
        (polyline
          (pts
            (xy -1.27 -2.54)
            (xy 1.27 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -2.54)
          )
          (fill (type none))
        )
        (pin power_in line (at 0 0 0) (length 0) hide
          (name "VCC3V3")
          (number "")
        )
      )
    )
    (symbol "WIFI-BT-altium-import:VCC_WIFI" (power) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 0 0))
      (property "Value" "VCC_WIFI" (id 1) (at 0 3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "电源符号创建名为 'VCC_WIFI' 的全局标签" (id 5) (at 0 0 0))
      (symbol "VCC_WIFI_0_0"
        (polyline
          (pts
            (xy -1.27 -2.54)
            (xy 1.27 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -2.54)
          )
          (fill (type none))
        )
        (pin power_in line (at 0 0 0) (length 0) hide
          (name "VCC_WIFI")
          (number "")
        )
      )
    )
  )
  (junction (at 58.42 113.4872) (diameter 0) (color 0 0 0 0))
  (junction (at 60.96 105.8672) (diameter 0) (color 0 0 0 0))
  (junction (at 132.08 161.7472) (diameter 0) (color 0 0 0 0))
  (junction (at 55.88 105.8672) (diameter 0) (color 0 0 0 0))
  (junction (at 137.16 161.7472) (diameter 0) (color 0 0 0 0))
  (junction (at 96.52 88.0872) (diameter 0) (color 0 0 0 0))
  (junction (at 134.62 161.7472) (diameter 0) (color 0 0 0 0))
  (junction (at 50.8 105.8672) (diameter 0) (color 0 0 0 0))
  (junction (at 144.78 161.7472) (diameter 0) (color 0 0 0 0))
  (junction (at 185.42 108.4072) (diameter 0) (color 0 0 0 0))
  (junction (at 175.26 85.5472) (diameter 0) (color 0 0 0 0))
  (junction (at 68.58 95.7072) (diameter 0) (color 0 0 0 0))
  (junction (at 127 151.5872) (diameter 0) (color 0 0 0 0))
  (junction (at 147.32 46.1772) (diameter 0) (color 0 0 0 0))
  (junction (at 152.4 138.8872) (diameter 0) (color 0 0 0 0))
  (junction (at 152.4 46.1772) (diameter 0) (color 0 0 0 0))
  (junction (at 142.24 161.7472) (diameter 0) (color 0 0 0 0))
  (junction (at 81.28 93.1672) (diameter 0) (color 0 0 0 0))
  (junction (at 81.28 88.0872) (diameter 0) (color 0 0 0 0))
  (junction (at 104.14 85.5472) (diameter 0) (color 0 0 0 0))
  (junction (at 152.4 152.8572) (diameter 0) (color 0 0 0 0))
  (no_connect (at 172.72 100.7872))
  (no_connect (at 106.68 110.9472))
  (no_connect (at 172.72 98.2472))
  (no_connect (at 162.56 65.2272))
  (no_connect (at 106.68 108.4072))
  (no_connect (at 172.72 103.3272))
  (no_connect (at 142.24 65.2272))
  (no_connect (at 137.16 65.2272))
  (no_connect (at 157.48 65.2272))
  (no_connect (at 106.68 93.1672))
  (no_connect (at 144.78 65.2272))
  (no_connect (at 149.86 131.2672))
  (no_connect (at 172.72 95.7072))
  (no_connect (at 172.72 88.0872))
  (no_connect (at 139.7 65.2272))
  (no_connect (at 172.72 110.9472))
  (no_connect (at 106.68 103.3272))
  (no_connect (at 106.68 95.7072))
  (no_connect (at 160.02 65.2272))
  (no_connect (at 172.72 105.8672))
  (wire (pts (xy 172.72 108.4072) (xy 185.42 108.4072)))
  (wire (pts (xy 142.24 161.7472) (xy 144.78 161.7472)))
  (wire (pts (xy 134.62 161.7472) (xy 137.16 161.7472)))
  (wire (pts (xy 132.08 131.2672) (xy 132.08 151.5872)))
  (wire (pts (xy 139.7 131.2672) (xy 139.7 166.8272)))
  (wire (pts (xy 45.72 105.8672) (xy 50.8 105.8672)))
  (wire (pts (xy 106.68 85.5472) (xy 104.14 85.5472)))
  (wire (pts (xy 152.4 161.7472) (xy 152.4 152.8572)))
  (wire (pts (xy 104.14 85.5472) (xy 104.14 90.6272)))
  (wire (pts (xy 86.36 100.7872) (xy 106.68 100.7872)))
  (wire (pts (xy 142.24 131.2672) (xy 142.24 151.5872)))
  (wire (pts (xy 55.88 113.4872) (xy 58.42 113.4872)))
  (wire (pts (xy 189.23 100.7872) (xy 185.42 100.7872)))
  (wire (pts (xy 60.96 108.4072) (xy 60.96 105.8672)))
  (wire (pts (xy 96.52 88.0872) (xy 106.68 88.0872)))
  (wire (pts (xy 50.8 105.8672) (xy 55.88 105.8672)))
  (wire (pts (xy 127 151.5872) (xy 127 131.2672)))
  (wire (pts (xy 127 65.2272) (xy 127 44.9072)))
  (wire (pts (xy 104.14 90.6272) (xy 106.68 90.6272)))
  (wire (pts (xy 152.4 65.2272) (xy 152.4 46.1772)))
  (wire (pts (xy 83.82 88.0872) (xy 81.28 88.0872)))
  (wire (pts (xy 93.98 88.0872) (xy 96.52 88.0872)))
  (wire (pts (xy 58.42 113.4872) (xy 60.96 113.4872)))
  (wire (pts (xy 127 161.7472) (xy 132.08 161.7472)))
  (wire (pts (xy 81.28 93.1672) (xy 81.28 95.7072)))
  (wire (pts (xy 60.96 105.8672) (xy 106.68 105.8672)))
  (wire (pts (xy 172.72 90.6272) (xy 175.26 90.6272)))
  (wire (pts (xy 182.88 93.1672) (xy 200.66 93.1672)))
  (wire (pts (xy 144.78 131.2672) (xy 144.78 151.5872)))
  (wire (pts (xy 144.78 161.7472) (xy 152.4 161.7472)))
  (wire (pts (xy 134.62 131.2672) (xy 134.62 151.5872)))
  (wire (pts (xy 175.26 85.5472) (xy 172.72 85.5472)))
  (wire (pts (xy 68.58 98.2472) (xy 68.58 95.7072)))
  (wire (pts (xy 132.08 65.2272) (xy 132.08 44.9072)))
  (wire (pts (xy 83.82 98.2472) (xy 106.68 98.2472)))
  (wire (pts (xy 152.4 46.1772) (xy 152.4 44.9072)))
  (wire (pts (xy 96.52 93.1672) (xy 81.28 93.1672)))
  (wire (pts (xy 119.38 151.5872) (xy 127 151.5872)))
  (wire (pts (xy 175.26 90.6272) (xy 175.26 85.5472)))
  (wire (pts (xy 185.42 100.7872) (xy 185.42 108.4072)))
  (wire (pts (xy 73.66 98.2472) (xy 68.58 98.2472)))
  (wire (pts (xy 137.16 131.2672) (xy 137.16 151.5872)))
  (wire (pts (xy 147.32 65.2272) (xy 147.32 46.1772)))
  (wire (pts (xy 81.28 95.7072) (xy 68.58 95.7072)))
  (wire (pts (xy 55.88 108.4072) (xy 55.88 105.8672)))
  (wire (pts (xy 129.54 65.2272) (xy 129.54 44.9072)))
  (wire (pts (xy 199.39 100.7872) (xy 210.82 100.7872)))
  (wire (pts (xy 129.54 131.2672) (xy 129.54 151.5872)))
  (wire (pts (xy 152.4 152.8572) (xy 152.4 138.8872)))
  (wire (pts (xy 55.88 105.8672) (xy 60.96 105.8672)))
  (wire (pts (xy 81.28 88.0872) (xy 73.66 88.0872)))
  (wire (pts (xy 134.62 46.1772) (xy 137.16 46.1772)))
  (wire (pts (xy 147.32 46.1772) (xy 147.32 44.9072)))
  (wire (pts (xy 185.42 108.4072) (xy 189.23 108.4072)))
  (wire (pts (xy 35.56 105.8672) (xy 30.48 105.8672)))
  (wire (pts (xy 152.4 138.8872) (xy 152.4 131.2672)))
  (wire (pts (xy 210.82 100.7872) (xy 210.82 93.1672)))
  (wire (pts (xy 132.08 161.7472) (xy 134.62 161.7472)))
  (wire (pts (xy 137.16 161.7472) (xy 142.24 161.7472)))
  (wire (pts (xy 134.62 65.2272) (xy 134.62 46.1772)))
  (wire (pts (xy 199.39 108.4072) (xy 210.82 108.4072)))
  (text "D" (at 160.02 52.07 180))
  (text "B" (at 123.19 158.75 180))
  (text "0.4~1.8Vpp" (at 173.99 110.9472 180))
  (text "B D mount" (at 80.01 150.3172 180))
  (text "XR829" (at 67.31 155.3972 180))
  (text "RTL8189" (at 67.31 147.7772 180))
  (text "C" (at 194.31 114.3 180))
  (text "此处交叉" (at 125.73 43.6372 180))
  (text "RTL8723DS" (at 67.31 150.3172 180))
  (text "A" (at 114.3 158.75 180))
  (text "A C mount" (at 80.01 156.6672 180))
  (label "UART1_TX" (at 129.54 56.9722 90))
  (label "UART1_RTS" (at 127 56.9722 90))
  (label "BT_WAKE_AP" (at 86.36 100.7872 0))
  (label "UART1_CTS" (at 134.62 56.9722 90))
  (label "PG1_SDC1_CMD" (at 137.16 151.5872 90))
  (label "UART1_RX" (at 132.08 56.9722 90))
  (label "PG11" (at 204.47 108.4072 0))
  (label "WL_REG_ON" (at 127 151.5872 90))
  (label "PG5_SDC1_D3" (at 134.62 151.5872 90))
  (label "AP-CLK24M-OUT" (at 182.88 93.1672 0))
  (label "WL_WAKE_AP" (at 129.54 151.5872 90))
  (label "PG0_SDC1_CLK" (at 139.7 151.5872 90))
  (label "AP_WAKE_BT" (at 86.36 98.2472 0))
  (label "PG2_SDC1_D0" (at 142.24 151.5872 90))
  (label "PG4_SDC1_D2" (at 132.08 151.5872 90))
  (label "BT_EN" (at 152.4 57.6072 90))
  (label "PG3_SDC1_D1" (at 144.78 151.5872 90))
  (symbol (lib_id "WIFI-BT-altium-import:2_CAP") (at 139.7 169.3672 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C18" (id 0) (at 141.986 170.3832 0))
    (property "Value" "NC" (id 1) (at 142.24 173.1772 0))
    (property "Footprint" "C0402" (id 2) (at 139.7 169.3672 0))
    (property "Datasheet" "" (id 3) (at 139.7 169.3672 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:1_RES") (at 119.38 162.0012 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R14" (id 0) (at 119.38 163.0172 90))
    (property "Value" "NC/100K" (id 1) (at 120.65 157.9372 90))
    (property "Footprint" "R0402" (id 2) (at 119.38 162.0012 0))
    (property "Datasheet" "" (id 3) (at 119.38 162.0012 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:VCC3V3") (at 152.4 152.8572 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 152.4 152.8572 0))
    (property "Value" "VCC3V3" (id 1) (at 156.21 152.8572 90))
    (property "Footprint" "" (id 2) (at 152.4 152.8572 0))
    (property "Datasheet" "" (id 3) (at 152.4 152.8572 0))
    (pin "")
  )
  (symbol (lib_id "WIFI-BT-altium-import:0_mirrored_RES") (at 199.644 108.4072 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R84" (id 0) (at 191.77 107.3912 0))
    (property "Value" "NC" (id 1) (at 191.77 111.9632 0))
    (property "Footprint" "R0402" (id 2) (at 199.644 108.4072 0))
    (property "Datasheet" "" (id 3) (at 199.644 108.4072 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:2_CAP") (at 96.52 90.6272 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C58" (id 0) (at 99.06 90.6272 0))
    (property "Value" "NC" (id 1) (at 99.06 93.1672 0))
    (property "Footprint" "C0402" (id 2) (at 96.52 90.6272 0))
    (property "Datasheet" "" (id 3) (at 96.52 90.6272 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:GND") (at 68.58 95.7072 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 68.58 95.7072 0))
    (property "Value" "GND" (id 1) (at 62.23 95.7072 90))
    (property "Footprint" "" (id 2) (at 68.58 95.7072 0))
    (property "Datasheet" "" (id 3) (at 68.58 95.7072 0))
    (pin "")
  )
  (symbol (lib_id "WIFI-BT-altium-import:1_RES") (at 142.24 162.0012 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R68" (id 0) (at 142.24 163.0172 90))
    (property "Value" "47K" (id 1) (at 143.51 157.9372 90))
    (property "Footprint" "R0402" (id 2) (at 142.24 162.0012 0))
    (property "Datasheet" "" (id 3) (at 142.24 162.0012 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:GND") (at 68.58 80.4672 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 68.58 80.4672 0))
    (property "Value" "GND" (id 1) (at 68.58 74.1172 0))
    (property "Footprint" "" (id 2) (at 68.58 80.4672 0))
    (property "Datasheet" "" (id 3) (at 68.58 80.4672 0))
    (pin "")
  )
  (symbol (lib_id "WIFI-BT-altium-import:VCC3V3") (at 30.48 105.8672 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 30.48 105.8672 0))
    (property "Value" "VCC3V3" (id 1) (at 30.48 102.0572 0))
    (property "Footprint" "" (id 2) (at 30.48 105.8672 0))
    (property "Datasheet" "" (id 3) (at 30.48 105.8672 0))
    (pin "")
  )
  (symbol (lib_id "WIFI-BT-altium-import:1_RES") (at 134.62 162.0012 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R66" (id 0) (at 134.62 163.0172 90))
    (property "Value" "47K" (id 1) (at 135.89 157.9372 90))
    (property "Footprint" "R0402" (id 2) (at 134.62 162.0012 0))
    (property "Datasheet" "" (id 3) (at 134.62 162.0012 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:2_RES") (at 84.074 98.2472 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R46" (id 0) (at 73.66 98.2472 0))
    (property "Value" "NC/100K" (id 1) (at 76.2 101.8032 0))
    (property "Footprint" "R0402" (id 2) (at 84.074 98.2472 0))
    (property "Datasheet" "" (id 3) (at 84.074 98.2472 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:VCC_WIFI") (at 50.8 105.8672 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 50.8 105.8672 0))
    (property "Value" "VCC_WIFI" (id 1) (at 50.8 102.0572 0))
    (property "Footprint" "" (id 2) (at 50.8 105.8672 0))
    (property "Datasheet" "" (id 3) (at 50.8 105.8672 0))
    (pin "")
  )
  (symbol (lib_id "WIFI-BT-altium-import:0_mirrored_RES") (at 162.814 46.1772 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R37" (id 0) (at 154.94 45.1612 0))
    (property "Value" "100K" (id 1) (at 154.94 49.7332 0))
    (property "Footprint" "R0402" (id 2) (at 162.814 46.1772 0))
    (property "Datasheet" "" (id 3) (at 162.814 46.1772 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:GND") (at 139.7 171.9072 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 139.7 171.9072 0))
    (property "Value" "GND" (id 1) (at 139.7 178.2572 0))
    (property "Footprint" "" (id 2) (at 139.7 171.9072 0))
    (property "Datasheet" "" (id 3) (at 139.7 171.9072 0))
    (pin "")
  )
  (symbol (lib_id "WIFI-BT-altium-import:GND") (at 175.26 85.5472 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 175.26 85.5472 0))
    (property "Value" "GND" (id 1) (at 181.61 85.5472 90))
    (property "Footprint" "" (id 2) (at 175.26 85.5472 0))
    (property "Datasheet" "" (id 3) (at 175.26 85.5472 0))
    (pin "")
  )
  (symbol (lib_id "WIFI-BT-altium-import:2_CAP") (at 81.28 90.6272 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C48" (id 0) (at 74.93 90.6272 0))
    (property "Value" "NC" (id 1) (at 74.93 93.1672 0))
    (property "Footprint" "C0402" (id 2) (at 81.28 90.6272 0))
    (property "Datasheet" "" (id 3) (at 81.28 90.6272 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:VCC3V3") (at 162.56 46.1772 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 162.56 46.1772 0))
    (property "Value" "VCC3V3" (id 1) (at 166.37 46.1772 90))
    (property "Footprint" "" (id 2) (at 162.56 46.1772 0))
    (property "Datasheet" "" (id 3) (at 162.56 46.1772 0))
    (pin "")
  )
  (symbol (lib_id "WIFI-BT-altium-import:GND") (at 119.38 161.7472 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 119.38 161.7472 0))
    (property "Value" "GND" (id 1) (at 119.38 168.0972 0))
    (property "Footprint" "" (id 2) (at 119.38 161.7472 0))
    (property "Datasheet" "" (id 3) (at 119.38 161.7472 0))
    (pin "")
  )
  (symbol (lib_id "WIFI-BT-altium-import:0_AP6212") (at 111.76 126.1872 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U6" (id 0) (at 173.228 70.3072 0))
    (property "Value" "WIFI" (id 1) (at 173.228 72.8472 0))
    (property "Footprint" "AP6212" (id 2) (at 111.76 126.1872 0))
    (property "Datasheet" "" (id 3) (at 111.76 126.1872 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "4")
    (pin "40")
    (pin "41")
    (pin "42")
    (pin "43")
    (pin "44")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "TP1")
    (pin "TP2")
    (pin "TP3")
  )
  (symbol (lib_id "WIFI-BT-altium-import:2_CAP") (at 60.96 110.9472 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C16" (id 0) (at 63.246 111.9632 0))
    (property "Value" "0.1uF" (id 1) (at 63.246 114.5032 0))
    (property "Footprint" "C0402" (id 2) (at 60.96 110.9472 0))
    (property "Datasheet" "" (id 3) (at 60.96 110.9472 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:1_RES") (at 137.16 162.0012 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R67" (id 0) (at 137.16 163.0172 90))
    (property "Value" "47K" (id 1) (at 138.43 157.9372 90))
    (property "Footprint" "R0402" (id 2) (at 137.16 162.0012 0))
    (property "Datasheet" "" (id 3) (at 137.16 162.0012 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:2_CAP") (at 55.88 110.9472 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C14" (id 0) (at 52.07 109.6772 0))
    (property "Value" "10uF" (id 1) (at 49.53 114.7572 0))
    (property "Footprint" "C0402" (id 2) (at 55.88 110.9472 0))
    (property "Datasheet" "" (id 3) (at 55.88 110.9472 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:2_RES") (at 94.234 88.0872 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R38" (id 0) (at 86.36 87.0712 0))
    (property "Value" "0R" (id 1) (at 88.9 89.3572 0))
    (property "Footprint" "R0402" (id 2) (at 94.234 88.0872 0))
    (property "Datasheet" "" (id 3) (at 94.234 88.0872 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:2_RES") (at 45.974 105.8672 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R58" (id 0) (at 38.1 104.8512 0))
    (property "Value" "0R" (id 1) (at 38.1 109.4232 0))
    (property "Footprint" "R0402" (id 2) (at 45.974 105.8672 0))
    (property "Datasheet" "" (id 3) (at 45.974 105.8672 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:3_CAP") (at 154.94 138.8872 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C19" (id 0) (at 153.416 136.6012 0))
    (property "Value" "1uF" (id 1) (at 153.416 143.7132 0))
    (property "Footprint" "C0402" (id 2) (at 154.94 138.8872 0))
    (property "Datasheet" "" (id 3) (at 154.94 138.8872 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:0_mirrored_RES") (at 147.574 46.1772 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R70" (id 0) (at 139.7 45.1612 0))
    (property "Value" "NC/100K" (id 1) (at 139.7 49.7332 0))
    (property "Footprint" "R0402" (id 2) (at 147.574 46.1772 0))
    (property "Datasheet" "" (id 3) (at 147.574 46.1772 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:GND") (at 147.32 44.9072 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 147.32 44.9072 0))
    (property "Value" "GND" (id 1) (at 147.32 38.5572 0))
    (property "Footprint" "" (id 2) (at 147.32 44.9072 0))
    (property "Datasheet" "" (id 3) (at 147.32 44.9072 0))
    (pin "")
  )
  (symbol (lib_id "WIFI-BT-altium-import:2_mirrored_RES") (at 188.976 100.7872 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R47" (id 0) (at 191.77 99.7712 0))
    (property "Value" "47K" (id 1) (at 191.77 104.3432 0))
    (property "Footprint" "R0402" (id 2) (at 188.976 100.7872 0))
    (property "Datasheet" "" (id 3) (at 188.976 100.7872 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:GND") (at 58.42 113.4872 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 58.42 113.4872 0))
    (property "Value" "GND" (id 1) (at 58.42 119.8372 0))
    (property "Footprint" "" (id 2) (at 58.42 113.4872 0))
    (property "Datasheet" "" (id 3) (at 58.42 113.4872 0))
    (pin "")
  )
  (symbol (lib_id "WIFI-BT-altium-import:GND") (at 157.48 138.8872 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 157.48 138.8872 0))
    (property "Value" "GND" (id 1) (at 163.83 138.8872 90))
    (property "Footprint" "" (id 2) (at 157.48 138.8872 0))
    (property "Datasheet" "" (id 3) (at 157.48 138.8872 0))
    (pin "")
  )
  (symbol (lib_id "WIFI-BT-altium-import:1_RES") (at 132.08 162.0012 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R65" (id 0) (at 132.08 163.0172 90))
    (property "Value" "47K" (id 1) (at 133.35 157.9372 90))
    (property "Footprint" "R0402" (id 2) (at 132.08 162.0012 0))
    (property "Datasheet" "" (id 3) (at 132.08 162.0012 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:0_mirrored_MCX_IPEX") (at 71.12 90.6272 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J4" (id 0) (at 74.168 85.2932 0))
    (property "Value" "ipex" (id 1) (at 74.168 87.8332 0))
    (property "Footprint" "I-PEX SOCKET" (id 2) (at 71.12 90.6272 0))
    (property "Datasheet" "" (id 3) (at 71.12 90.6272 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "WIFI-BT-altium-import:2_RES") (at 183.134 93.1672 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R41" (id 0) (at 175.26 92.1512 0))
    (property "Value" "NC/0R" (id 1) (at 175.26 96.7232 0))
    (property "Footprint" "R0402" (id 2) (at 183.134 93.1672 0))
    (property "Datasheet" "" (id 3) (at 183.134 93.1672 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:GND") (at 147.32 131.2672 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 147.32 131.2672 0))
    (property "Value" "GND" (id 1) (at 147.32 137.6172 0))
    (property "Footprint" "" (id 2) (at 147.32 131.2672 0))
    (property "Datasheet" "" (id 3) (at 147.32 131.2672 0))
    (pin "")
  )
  (symbol (lib_id "WIFI-BT-altium-import:1_RES") (at 127 162.0012 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R5" (id 0) (at 127 161.7472 90))
    (property "Value" "100K" (id 1) (at 128.27 157.9372 90))
    (property "Footprint" "R0402" (id 2) (at 127 162.0012 0))
    (property "Datasheet" "" (id 3) (at 127 162.0012 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "WIFI-BT-altium-import:VCC3V3") (at 210.82 93.1672 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 210.82 93.1672 0))
    (property "Value" "VCC3V3" (id 1) (at 210.82 89.3572 0))
    (property "Footprint" "" (id 2) (at 210.82 93.1672 0))
    (property "Datasheet" "" (id 3) (at 210.82 93.1672 0))
    (pin "")
  )
  (symbol (lib_id "WIFI-BT-altium-import:GND") (at 104.14 85.5472 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 104.14 85.5472 0))
    (property "Value" "GND" (id 1) (at 104.14 79.1972 0))
    (property "Footprint" "" (id 2) (at 104.14 85.5472 0))
    (property "Datasheet" "" (id 3) (at 104.14 85.5472 0))
    (pin "")
  )
  (symbol (lib_id "WIFI-BT-altium-import:1_RES") (at 144.78 162.0012 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R69" (id 0) (at 144.78 163.0172 90))
    (property "Value" "47K" (id 1) (at 146.05 157.9372 90))
    (property "Footprint" "R0402" (id 2) (at 144.78 162.0012 0))
    (property "Datasheet" "" (id 3) (at 144.78 162.0012 0))
    (pin "1")
    (pin "2")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC_WIFI") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC3V3") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "C14") (unit 1) (value "10uF") (footprint "C0402")
    )
    (path
      (reference "C16") (unit 1) (value "0.1uF") (footprint "C0402")
    )
    (path
      (reference "C18") (unit 1) (value "NC") (footprint "C0402")
    )
    (path
      (reference "C19") (unit 1) (value "1uF") (footprint "C0402")
    )
    (path
      (reference "C48") (unit 1) (value "NC") (footprint "C0402")
    )
    (path
      (reference "C58") (unit 1) (value "NC") (footprint "C0402")
    )
    (path
      (reference "J4") (unit 1) (value "ipex") (footprint "I-PEX SOCKET")
    )
    (path
      (reference "R5") (unit 1) (value "100K") (footprint "R0402")
    )
    (path
      (reference "R14") (unit 1) (value "NC/100K") (footprint "R0402")
    )
    (path
      (reference "R37") (unit 1) (value "100K") (footprint "R0402")
    )
    (path
      (reference "R38") (unit 1) (value "0R") (footprint "R0402")
    )
    (path
      (reference "R41") (unit 1) (value "NC/0R") (footprint "R0402")
    )
    (path
      (reference "R46") (unit 1) (value "NC/100K") (footprint "R0402")
    )
    (path
      (reference "R47") (unit 1) (value "47K") (footprint "R0402")
    )
    (path
      (reference "R58") (unit 1) (value "0R") (footprint "R0402")
    )
    (path
      (reference "R65") (unit 1) (value "47K") (footprint "R0402")
    )
    (path
      (reference "R66") (unit 1) (value "47K") (footprint "R0402")
    )
    (path
      (reference "R67") (unit 1) (value "47K") (footprint "R0402")
    )
    (path
      (reference "R68") (unit 1) (value "47K") (footprint "R0402")
    )
    (path
      (reference "R69") (unit 1) (value "47K") (footprint "R0402")
    )
    (path
      (reference "R70") (unit 1) (value "NC/100K") (footprint "R0402")
    )
    (path
      (reference "R84") (unit 1) (value "NC") (footprint "R0402")
    )
    (path
      (reference "U6") (unit 1) (value "WIFI") (footprint "AP6212")
    )
  )
)
